; Version 1.1   10/24/91
AdapterId 0FE92h
 				
;AdapterName "IBM PS/2 System/370 Channel Adapter"
Adaptername "IBM PS/2 Block Multiplxer Adapter"  
 
NumBytes 6
 
fixedresources
        pos[0]=xxxxxxxxb
        pos[1]=xxxxxxxxb
        pos[2]=10111xxxb
        pos[3]=xxxxxxxxb
        pos[4]=xxxxxxxxb
        pos[5]=xxxxxxxxb
 
nameditem
        prompt "Shared RAM Address"
        Choice  "000F80000h - 000FBFFFFh"
                pos[0]=0010xxxxb
                mem 000F80000h - 000FBFFFFh
        Choice  "001100000h - 00113FFFFh"
                pos[0]=0101xxxxb
                mem 001100000h - 00113FFFFh
        Choice  "001200000h - 00123FFFFh"
                pos[0]=0110xxxxb
                mem 001200000h - 00123FFFFh
        Choice  "001300000h - 00133FFFFh"
                pos[0]=0111xxxxb
                mem 001300000h - 00133FFFFh
        Choice  "001400000h - 00143FFFFh"
                pos[0]=1000xxxxb
                mem 001400000h - 00143FFFFh
        Choice  "001500000h - 00153FFFFh"
                pos[0]=1001xxxxb
                mem 001500000h - 00153FFFFh
        Choice  "001600000h - 00163FFFFh"
                pos[0]=1010xxxxb
                mem 001600000h - 00163FFFFh
        Choice  "001700000h - 00173FFFFh"
                pos[0]=1011xxxxb
                mem 001700000h - 00173FFFFh
        Choice  "0FFC00000h - 0FFC3FFFFh"
                pos[0]=1100xxxxb
                mem 0FFC00000h - 0FFC3FFFFh
        Choice  "0FFD00000h - 0FFD3FFFFh"
                pos[0]=1101xxxxb
                mem 0FFD00000h - 0FFD3FFFFh
        Choice  "0FFE00000h - 0FFE3FFFFh"
                pos[0]=1110xxxxb
                mem 0FFE00000h - 0FFE3FFFFh
        Choice  "000800000h - 00083FFFFh"
                pos[0]=0000xxxxb
                mem 000800000h - 00083FFFFh
        Choice  "000F40000h - 000F7FFFFh"
                pos[0]=0001xxxxb
                mem 000F40000h - 000F7FFFFh
        Choice  "000FC0000h - 000FFFFFFh"
                pos[0]=0011xxxxb
                mem 000FC0000h - 000FFFFFFh
        Help
        "Selects the location of the RAM Memory used by the adapter.
Normally set to 000F80000h 000FBFFFFh."
 
nameditem
        prompt "Interrupt level"
        choice "11"
                pos[3]=xxxxx110b
                int 11
        choice "10"
                pos[3]=xxxxx101b
                int 10
        choice "9"
                pos[3]=xxxxx100b
                int 9
        choice "7"
                pos[3]=xxxxx011b
                int 7
        choice "6"
                pos[3]=xxxxx010b
                int 6
        choice "5"
                pos[3]=xxxxx001b
                int 5
        choice "4"
                pos[3]=xxxxx000b
                int 4
        choice "14"
                pos[3]=xxxxx111b
                int 14
        Help
        "Selects the interrupt vector used by the adapter.
Normally set to 11."
 
