;*****************************************************************************
;*                       Tiara Computer Systems, Inc.                        *
;*         2700 Garcia Avenue  Mountain View, California  94043              *
;*              LANcard/A-II ARCnet Adapter Configuration File               *
;*                     Part #70-00366-3000     ECO #292                      *
;*                                                                           *
;*   Source File: @5F60.ASC                                                  *
;*   Engineer: William Karwacki - Hardware Engineering                       *
;*   Concurrance: Barry Rose - Technical Support                             *
;*                                                                           *
;*****************************************************************************

        adapterid 05F60h

        adaptername "Tiara Local Area Networks LANcard/A-II ARCnet Adapter"

        numbytes 4

        nameditem
                prompt "Node Identification Select"
                        choice "Node Address= 000 (000 hex)"
                                pos[2]=00000000b
                        choice "Node Address= 001 (001 hex)"
                                pos[2]=00000001b
                        choice "Node Address= 002 (002 hex)"
                                pos[2]=00000010b
                        choice "Node Address= 003 (003 hex)"
                                pos[2]=00000011b
                        choice "Node Address= 004 (004 hex)"
                                pos[2]=00000100b
                        choice "Node Address= 005 (005 hex)"
                                pos[2]=00000101b
                        choice "Node Address= 006 (006 hex)"
                                pos[2]=00000110b
                        choice "Node Address= 007 (007 hex)"
                                pos[2]=00000111b
                        choice "Node Address= 008 (008 hex)"
                                pos[2]=00001000b
                        choice "Node Address= 009 (009 hex)"
                                pos[2]=00001001b
                        choice "Node Address= 010 (00A hex)"
                                pos[2]=00001010b
                        choice "Node Address= 011 (00B hex)"
                                pos[2]=00001011b
                        choice "Node Address= 012 (00C hex)"
                                pos[2]=00001100b
                        choice "Node Address= 013 (00D hex)"
                                pos[2]=00001101b
                        choice "Node Address= 014 (00E hex)"
                                pos[2]=00001110b
                        choice "Node Address= 015 (00F hex)"
                                pos[2]=00001111b
                        choice "Node Address= 016 (010 hex)"
                                pos[2]=00010000b
                        choice "Node Address= 017 (011 hex)"
                                pos[2]=00010001b
                        choice "Node Address= 018 (012 hex)"
                                pos[2]=00010010b
                        choice "Node Address= 019 (013 hex)"
                                pos[2]=00010011b
                        choice "Node Address= 020 (014 hex)"
                                pos[2]=00010100b
                        choice "Node Address= 021 (015 hex)"
                                pos[2]=00010101b
                        choice "Node Address= 022 (016 hex)"
                                pos[2]=00010110b
                        choice "Node Address= 023 (017 hex)"
                                pos[2]=00010111b
                        choice "Node Address= 024 (018 hex)"
                                pos[2]=00011000b
                        choice "Node Address= 025 (019 hex)"
                                pos[2]=00011001b
                        choice "Node Address= 026 (01A hex)"
                                pos[2]=00011010b
                        choice "Node Address= 027 (01B hex)"
                                pos[2]=00011011b
                        choice "Node Address= 028 (01C hex)"
                                pos[2]=00011100b
                        choice "Node Address= 029 (01D hex)"
                                pos[2]=00011101b
                        choice "Node Address= 030 (01E hex)"
                                pos[2]=00011110b
                        choice "Node Address= 031 (01F hex)"
                                pos[2]=00011111b
                        choice "Node Address= 032 (020 hex)"
                                pos[2]=00100000b
                        choice "Node Address= 033 (021 hex)"
                                pos[2]=00100001b
                        choice "Node Address= 034 (022 hex)"
                                pos[2]=00100010b
                        choice "Node Address= 035 (023 hex)"
                                pos[2]=00100011b
                        choice "Node Address= 036 (024 hex)"
                                pos[2]=00100100b
                        choice "Node Address= 037 (025 hex)"
                                pos[2]=00100101b
                        choice "Node Address= 038 (026 hex)"
                                pos[2]=00100110b
                        choice "Node Address= 039 (027 hex)"
                                pos[2]=00100111b
                        choice "Node Address= 040 (028 hex)"
                                pos[2]=00101000b
                        choice "Node Address= 041 (029 hex)"
                                pos[2]=00101001b
                        choice "Node Address= 042 (02A hex)"
                                pos[2]=00101010b
                        choice "Node Address= 043 (02B hex)"
                                pos[2]=00101011b
                        choice "Node Address= 044 (02C hex)"
                                pos[2]=00101100b
                        choice "Node Address= 045 (02D hex)"
                                pos[2]=00101101b
                        choice "Node Address= 046 (02E hex)"
                                pos[2]=00101110b
                        choice "Node Address= 047 (02F hex)"
                                pos[2]=00101111b
                        choice "Node Address= 048 (030 hex)"
                                pos[2]=00110000b
                        choice "Node Address= 049 (031 hex)"
                                pos[2]=00110001b
                        choice "Node Address= 050 (032 hex)"
                                pos[2]=00110010b
                        choice "Node Address= 051 (033 hex)"
                                pos[2]=00110011b
                        choice "Node Address= 052 (034 hex)"
                                pos[2]=00110100b
                        choice "Node Address= 053 (035 hex)"
                                pos[2]=00110101b
                        choice "Node Address= 054 (036 hex)"
                                pos[2]=00110110b
                        choice "Node Address= 055 (037 hex)"
                                pos[2]=00110111b
                        choice "Node Address= 056 (038 hex)"
                                pos[2]=00111000b
                        choice "Node Address= 057 (039 hex)"
                                pos[2]=00111001b
                        choice "Node Address= 058 (03A hex)"
                                pos[2]=00111010b
                        choice "Node Address= 059 (03B hex)"
                                pos[2]=00111011b
                        choice "Node Address= 060 (03C hex)"
                                pos[2]=00111100b
                        choice "Node Address= 061 (03D hex)"
                                pos[2]=00111101b
                        choice "Node Address= 062 (03E hex)"
                                pos[2]=00111110b
                        choice "Node Address= 063 (03F hex)"
                                pos[2]=00111111b
                        choice "Node Address= 064 (040 hex)"
                                pos[2]=01000000b
                        choice "Node Address= 065 (041 hex)"
                                pos[2]=01000001b
                        choice "Node Address= 066 (042 hex)"
                                pos[2]=01000010b
                        choice "Node Address= 067 (043 hex)"
                                pos[2]=01000011b
                        choice "Node Address= 068 (044 hex)"
                                pos[2]=01000100b
                        choice "Node Address= 069 (045 hex)"
                                pos[2]=01000101b
                        choice "Node Address= 070 (046 hex)"
                                pos[2]=01000110b
                        choice "Node Address= 071 (047 hex)"
                                pos[2]=01000111b
                        choice "Node Address= 072 (048 hex)"
                                pos[2]=01001000b
                        choice "Node Address= 073 (049 hex)"
                                pos[2]=01001001b
                        choice "Node Address= 074 (04A hex)"
                                pos[2]=01001010b
                        choice "Node Address= 075 (04B hex)"
                                pos[2]=01001011b
                        choice "Node Address= 076 (04C hex)"
                                pos[2]=01001100b
                        choice "Node Address= 077 (04D hex)"
                                pos[2]=01001101b
                        choice "Node Address= 078 (04E hex)"
                                pos[2]=01001110b
                        choice "Node Address= 079 (04F hex)"
                                pos[2]=01001111b
                        choice "Node Address= 080 (050 hex)"
                                pos[2]=01010000b
                        choice "Node Address= 081 (051 hex)"
                                pos[2]=01010001b
                        choice "Node Address= 082 (052 hex)"
                                pos[2]=01010010b
                        choice "Node Address= 083 (053 hex)"
                                pos[2]=01010011b
                        choice "Node Address= 084 (054 hex)"
                                pos[2]=01010100b
                        choice "Node Address= 085 (055 hex)"
                                pos[2]=01010101b
                        choice "Node Address= 086 (056 hex)"
                                pos[2]=01010110b
                        choice "Node Address= 087 (057 hex)"
                                pos[2]=01010111b
                        choice "Node Address= 088 (058 hex)"
                                pos[2]=01011000b
                        choice "Node Address= 089 (059 hex)"
                                pos[2]=01011001b
                        choice "Node Address= 090 (05A hex)"
                                pos[2]=01011010b
                        choice "Node Address= 091 (05B hex)"
                                pos[2]=01011011b
                        choice "Node Address= 092 (05C hex)"
                                pos[2]=01011100b
                        choice "Node Address= 093 (05D hex)"
                                pos[2]=01011101b
                        choice "Node Address= 094 (05E hex)"
                                pos[2]=01011110b
                        choice "Node Address= 095 (05F hex)"
                                pos[2]=01011111b
                        choice "Node Address= 096 (060 hex)"
                                pos[2]=01100000b
                        choice "Node Address= 097 (061 hex)"
                                pos[2]=01100001b
                        choice "Node Address= 098 (062 hex)"
                                pos[2]=01100010b
                        choice "Node Address= 099 (063 hex)"
                                pos[2]=01100011b
                        choice "Node Address= 100 (064 hex)"
                                pos[2]=01100100b
                        choice "Node Address= 101 (065 hex)"
                                pos[2]=01100101b
                        choice "Node Address= 102 (066 hex)"
                                pos[2]=01100110b
                        choice "Node Address= 103 (067 hex)"
                                pos[2]=01100111b
                        choice "Node Address= 104 (068 hex)"
                                pos[2]=01101000b
                        choice "Node Address= 105 (069 hex)"
                                pos[2]=01101001b
                        choice "Node Address= 106 (06A hex)"
                                pos[2]=01101010b
                        choice "Node Address= 107 (06B hex)"
                                pos[2]=01101011b
                        choice "Node Address= 108 (06C hex)"
                                pos[2]=01101100b
                        choice "Node Address= 109 (06D hex)"
                                pos[2]=01101101b
                        choice "Node Address= 110 (06E hex)"
                                pos[2]=01101110b
                        choice "Node Address= 111 (06F hex)"
                                pos[2]=01101111b
                        choice "Node Address= 112 (070 hex)"
                                pos[2]=01110000b
                        choice "Node Address= 113 (071 hex)"
                                pos[2]=01110001b
                        choice "Node Address= 114 (072 hex)"
                                pos[2]=01110010b
                        choice "Node Address= 115 (073 hex)"
                                pos[2]=01110011b
                        choice "Node Address= 116 (074 hex)"
                                pos[2]=01110100b
                        choice "Node Address= 117 (075 hex)"
                                pos[2]=01110101b
                        choice "Node Address= 118 (076 hex)"
                                pos[2]=01110110b
                        choice "Node Address= 119 (077 hex)"
                                pos[2]=01110111b
                        choice "Node Address= 120 (078 hex)"
                                pos[2]=01111000b
                        choice "Node Address= 121 (079 hex)"
                                pos[2]=01111001b
                        choice "Node Address= 122 (07A hex)"
                                pos[2]=01111010b
                        choice "Node Address= 123 (07B hex)"
                                pos[2]=01111011b
                        choice "Node Address= 124 (07C hex)"
                                pos[2]=01111100b
                        choice "Node Address= 125 (07D hex)"
                                pos[2]=01111101b
                        choice "Node Address= 126 (07E hex)"
                                pos[2]=01111110b
                        choice "Node Address= 127 (07F hex)"
                                pos[2]=01111111b
                        choice "Node Address= 128 (080 hex)"
                                pos[2]=10000000b
                        choice "Node Address= 129 (081 hex)"
                                pos[2]=10000001b
                        choice "Node Address= 130 (082 hex)"
                                pos[2]=10000010b
                        choice "Node Address= 131 (083 hex)"
                                pos[2]=10000011b
                        choice "Node Address= 132 (084 hex)"
                                pos[2]=10000100b
                        choice "Node Address= 133 (085 hex)"
                                pos[2]=10000101b
                        choice "Node Address= 134 (086 hex)"
                                pos[2]=10000110b
                        choice "Node Address= 135 (087 hex)"
                                pos[2]=10000111b
                        choice "Node Address= 136 (088 hex)"
                                pos[2]=10001000b
                        choice "Node Address= 137 (089 hex)"
                                pos[2]=10001001b
                        choice "Node Address= 138 (08A hex)"
                                pos[2]=10001010b
                        choice "Node Address= 139 (08B hex)"
                                pos[2]=10001011b
                        choice "Node Address= 140 (08C hex)"
                                pos[2]=10001100b
                        choice "Node Address= 141 (08D hex)"
                                pos[2]=10001101b
                        choice "Node Address= 142 (08E hex)"
                                pos[2]=10001110b
                        choice "Node Address= 143 (08F hex)"
                                pos[2]=10001111b
                        choice "Node Address= 144 (090 hex)"
                                pos[2]=10010000b
                        choice "Node Address= 145 (091 hex)"
                                pos[2]=10010001b
                        choice "Node Address= 146 (092 hex)"
                                pos[2]=10010010b
                        choice "Node Address= 147 (093 hex)"
                                pos[2]=10010011b
                        choice "Node Address= 148 (094 hex)"
                                pos[2]=10010100b
                        choice "Node Address= 149 (095 hex)"
                                pos[2]=10010101b
                        choice "Node Address= 150 (096 hex)"
                                pos[2]=10010110b
                        choice "Node Address= 151 (097 hex)"
                                pos[2]=10010111b
                        choice "Node Address= 152 (098 hex)"
                                pos[2]=10011000b
                        choice "Node Address= 153 (099 hex)"
                                pos[2]=10011001b
                        choice "Node Address= 154 (09A hex)"
                                pos[2]=10011010b
                        choice "Node Address= 155 (09B hex)"
                                pos[2]=10011011b
                        choice "Node Address= 156 (09C hex)"
                                pos[2]=10011100b
                        choice "Node Address= 157 (09D hex)"
                                pos[2]=10011101b
                        choice "Node Address= 158 (09E hex)"
                                pos[2]=10011110b
                        choice "Node Address= 159 (09F hex)"
                                pos[2]=10011111b
                        choice "Node Address= 160 (0A0 hex)"
                                pos[2]=10100000b
                        choice "Node Address= 161 (0A1 hex)" 
                                pos[2]=10100001b
                        choice "Node Address= 162 (0A2 hex)"
                                pos[2]=10100010b
                        choice "Node Address= 163 (0A3 hex)"
                                pos[2]=10100011b
                        choice "Node Address= 164 (0A4 hex)"
                                pos[2]=10100100b
                        choice "Node Address= 165 (0A5 hex)"
                                pos[2]=10100101b
                        choice "Node Address= 166 (0A6 hex)"
                                pos[2]=10100110b
                        choice "Node Address= 167 (0A7 hex)"
                                pos[2]=10100111b
                        choice "Node Address= 168 (0A8 hex)"
                                pos[2]=10101000b
                        choice "Node Address= 169 (0A9 hex)"
                                pos[2]=10101001b
                        choice "Node Address= 170 (0AA hex)"
                                pos[2]=10101010b
                        choice "Node Address= 171 (0AB hex)"
                                pos[2]=10101011b
                        choice "Node Address= 172 (0AC hex)"
                                pos[2]=10101100b
                        choice "Node Address= 173 (0AD hex)"
                                pos[2]=10101101b
                        choice "Node Address= 174 (0AE hex)"
                                pos[2]=10101110b
                        choice "Node Address= 175 (0AF hex)"
                                pos[2]=10101111b
                        choice "Node Address= 176 (0B0 hex)"
                                pos[2]=10110000b
                        choice "Node Address= 177 (0B1 hex)"
                                pos[2]=10110001b
                        choice "Node Address= 178 (0B2 hex)"
                                pos[2]=10110010b
                        choice "Node Address= 179 (0B3 hex)"
                                pos[2]=10110011b
                        choice "Node Address= 180 (0B4 hex)"
                                pos[2]=10110100b
                        choice "Node Address= 181 (0B5 hex)"
                                pos[2]=10110101b
                        choice "Node Address= 182 (0B6 hex)"
                                pos[2]=10110110b
                        choice "Node Address= 183 (0B7 hex)"
                                pos[2]=10110111b
                        choice "Node Address= 184 (0B8 hex)"
                                pos[2]=10111000b
                        choice "Node Address= 185 (0B9 hex)"
                                pos[2]=10111001b
                        choice "Node Address= 186 (0BA hex)"
                                pos[2]=10111010b
                        choice "Node Address= 187 (0BB hex)"
                                pos[2]=10111011b
                        choice "Node Address= 188 (0BC hex)"
                                pos[2]=10111100b
                        choice "Node Address= 189 (0BD hex)"
                                pos[2]=10111101b
                        choice "Node Address= 190 (0BE hex)"
                                pos[2]=10111110b
                        choice "Node Address= 191 (0BF hex)"
                                pos[2]=10111111b
                        choice "Node Address= 192 (0C0 hex)"
                                pos[2]=11000000b
                        choice "Node Address= 193 (0C1 hex)"
                                pos[2]=11000001b
                        choice "Node Address= 194 (0C2 hex)"
                                pos[2]=11000010b
                        choice "Node Address= 195 (0C3 hex)"
                                pos[2]=11000011b
                        choice "Node Address= 196 (0C4 hex)"
                                pos[2]=11000100b
                        choice "Node Address= 197 (0C5 hex)"
                                pos[2]=11000101b
                        choice "Node Address= 198 (0C6 hex)"
                                pos[2]=11000110b
                        choice "Node Address= 199 (0C7 hex)"
                                pos[2]=11000111b
                        choice "Node Address= 200 (0C8 hex)"
                                pos[2]=11001000b
                        choice "Node Address= 201 (0C9 hex)"
                                pos[2]=11001001b
                        choice "Node Address= 202 (0CA hex)"
                                pos[2]=11001010b
                        choice "Node Address= 203 (0CB hex)"
                                pos[2]=11001011b
                        choice "Node Address= 204 (0CC hex)"
                                pos[2]=11001100b
                        choice "Node Address= 205 (0CD hex)"
                                pos[2]=11001101b
                        choice "Node Address= 206 (0CE hex)"
                                pos[2]=11001110b
                        choice "Node Address= 207 (0CF hex)"
                                pos[2]=11001111b
                        choice "Node Address= 208 (0D0 hex)"
                                pos[2]=11010000b
                        choice "Node Address= 209 (0D1 hex)"
                                pos[2]=11010001b
                        choice "Node Address= 210 (0D2 hex)"
                                pos[2]=11010010b
                        choice "Node Address= 211 (0D3 hex)"
                                pos[2]=11010011b
                        choice "Node Address= 212 (0D4 hex)"
                                pos[2]=11010100b
                        choice "Node Address= 213 (0D5 hex)"
                                pos[2]=11010101b
                        choice "Node Address= 214 (0D6 hex)"
                                pos[2]=11010110b
                        choice "Node Address= 215 (0D7 hex)"
                                pos[2]=11010111b
                        choice "Node Address= 216 (0D8 hex)"
                                pos[2]=11011000b
                        choice "Node Address= 217 (0D9 hex)"
                                pos[2]=11011001b
                        choice "Node Address= 218 (0DA hex)"
                                pos[2]=11011010b
                        choice "Node Address= 219 (0DB hex)"
                                pos[2]=11011011b
                        choice "Node Address= 220 (0DC hex)"
                                pos[2]=11011100b
                        choice "Node Address= 221 (0DD hex)"
                                pos[2]=11011101b
                        choice "Node Address= 222 (0DE hex)"
                                pos[2]=11011110b
                        choice "Node Address= 223 (0DF hex)"
                                pos[2]=11011111b
                        choice "Node Address= 224 (0E0 hex)"
                                pos[2]=11100000b
                        choice "Node Address= 225 (0E1 hex)"
                                pos[2]=11100001b
                        choice "Node Address= 226 (0E2 hex)"
                                pos[2]=11100010b
                        choice "Node Address= 227 (0E3 hex)"
                                pos[2]=11100011b
                        choice "Node Address= 228 (0E4 hex)"
                                pos[2]=11100100b
                        choice "Node Address= 229 (0E5 hex)"
                                pos[2]=11100101b
                        choice "Node Address= 230 (0E6 hex)"
                                pos[2]=11100110b
                        choice "Node Address= 231 (0E7 hex)"
                                pos[2]=11100111b
                        choice "Node Address= 232 (0E8 hex)"
                                pos[2]=11101000b
                        choice "Node Address= 233 (0E9 hex)"
                                pos[2]=11101001b
                        choice "Node Address= 234 (0EA hex)"
                                pos[2]=11101010b
                        choice "Node Address= 235 (0EB hex)"
                                pos[2]=11101011b
                        choice "Node Address= 236 (0EC hex)"
                                pos[2]=11101100b
                        choice "Node Address= 237 (0ED hex)"
                                pos[2]=11101101b
                        choice "Node Address= 238 (0EE hex)"
                                pos[2]=11101110b
                        choice "Node Address= 239 (0EF hex)"
                                pos[2]=11101111b
                        choice "Node Address= 240 (0F0 hex)"
                                pos[2]=11110000b
                        choice "Node Address= 241 (0F1 hex)"
                                pos[2]=11110001b
                        choice "Node Address= 242 (0F2 hex)"
                                pos[2]=11110010b
                        choice "Node Address= 243 (0F3 hex)"
                                pos[2]=11110011b
                        choice "Node Address= 244 (0F4 hex)"
                                pos[2]=11110100b
                        choice "Node Address= 245 (0F5 hex)"
                                pos[2]=11110101b
                        choice "Node Address= 246 (0F6 hex)"
                                pos[2]=11110110b
                        choice "Node Address= 247 (0F7 hex)"
                                pos[2]=11110111b
                        choice "Node Address= 248 (0F8 hex)"
                                pos[2]=11111000b
                        choice "Node Address= 249 (0F9 hex)"
                                pos[2]=11111001b
                        choice "Node Address= 250 (0FA hex)"
                                pos[2]=11111010b
                        choice "Node Address= 251 (0FB hex)"
                                pos[2]=11111011b
                        choice "Node Address= 252 (0FC hex)"
                                pos[2]=11111100b
                        choice "Node Address= 253 (0FD hex)"
                                pos[2]=11111101b
                        choice "Node Address= 254 (0FE hex)"
                                pos[2]=11111110b
                        choice "Node Address= 255 (0FF hex)" 
                                pos[2]=11111111b
                help
                        "In order to access the network, a node address must be
assigned to this station. It is critical that the address selected be unique and
non-zero.  Please note that it is not possible for this configuration utility to determine if
the address selected is unique. Once an available node ID has been determined, hold the F5 or F6
key depressed to quickly scroll through the possible node addresses."

        nameditem
                prompt "RIM Buffer Base Address Offset Select"
                        choice "Offset 0D000"
                                pos[1]=XXXX1000b
                                mem 0D0000h-0D07FFh
                        choice "Offset 0D200"
                                pos[1]=XXXX1001b
                                mem 0D2000h-0D27FFh
                        choice "Offset 0D400"
                                pos[1]=XXXX1010b
                                mem 0D4000h-0D47FFh
                        choice "Offset 0D600"
                                pos[1]=XXXX1011b
                                mem 0D6000h-0D7FFFh
                        choice "Offset 0D800"
                                pos[1]=XXXX1100b
                                mem 0D8000h-0D87FFh
                        choice "Offset 0DA00"
                                pos[1]=XXXX1101b
                                mem 0DA000h-0DA7FFh
                        choice "Offset 0DC00"
                                pos[1]=XXXX1110b
                                mem 0DC000h-0DC7FFh
                        choice "Offset 0DE00"
                                pos[1]=XXXX1111b
                                mem 0DE000h-0DE7FFh
                        choice "Offset 0C000"
                                pos[1]=XXXX0000b
                                mem 0C0000h-0C07FFh
                        choice "Offset 0C200"
                                pos[1]=XXXX0001b
                                mem 0C2000h-0C27FFh
                        choice "Offset 0C400"
                                pos[1]=XXXX0010b
                                mem 0C4000h-0C47FFh
                        choice "Offset 0C600"
                                pos[1]=XXXX0011b
                                mem 0C6000h-0C7FFFh
                        choice "Offset 0C800"
                                pos[1]=XXXX0100b
                                mem 0C8000h-0C87FFh
                        choice "Offset 0CA00"
                                pos[1]=XXXX0101b
                                mem 0CA000h-0CA7FFh
                        choice "Offset 0CC00"
                                pos[1]=XXXX0110b
                                mem 0CC000h-0CC7FFh
                        choice "Offset 0CE00"
                                pos[1]=XXXX0111b
                                mem 0CE000h-0CE7FFh
                help
                        "In order for the RIM buffer to reside with any other
expansion RAM/ROM in the PS/2, a nonconflicting base address must be selected.
A conflict condition is indicated with an asterisk (*) at end of the base address
offset selected. Make note of the base address selected so that the proper network
shell can be installed. The default setting is offset 0D000."

        nameditem
                prompt "Base I/O Port Address Select"
                        choice "Base I/O Port 02E0"
                                pos[0]=XXXX001Xb
                                io 02E0h-02EFh
                        choice "Base I/O Port 02F0"
                                pos[0]=XXXX010Xb
                                io 02F0h-02FFh
                        choice "Base I/O Port 0300"
                                pos[0]=XXXX011Xb
                                io 0300h-030Fh
                        choice "Base I/O Port 1280"
                                pos[0]=XXXX100Xb
                                io 1280h-128Fh
                        choice "Base I/O Port 12E0"
                                pos[0]=XXXX101Xb
                                io 12E0h-12EFh
                        choice "Base I/O Port 12F0"
                                pos[0]=XXXX110Xb
                                io 12F0h-12FFh
                        choice "Base I/O Port 72E0"
                                pos[0]=XXXX111Xb
                                io 72E0h-72EFh
                        choice "Base I/O Port 0280"
                                pos[0]=XXXX000Xb
                                io 0280h-028Fh
                help
                        "In order for the LANcard/A-II to operate in the PS/2,
a nonconflicting base I/O port address must be selected. Under ordinary circumstances,
select the default address 02E0. A conflict condition is indicated with an asterisk (*)
at end of the base I/O port selected. Make note of the base port selected so that the
proper network shell can be installed."

        nameditem
                prompt "Interrupt Request Level Select"
                        choice "Interrupt Request IRQ2"
                                pos[3]=XXXXX000b
                                int 2
                        choice "Interrupt Request IRQ3"
                                pos[3]=XXXXX001b
                                int 3
                        choice "Interrupt Request IRQ4"
                                pos[3]=XXXXX010b
                                int 4
                        choice "Interrupt Request IRQ6"
                                pos[3]=XXXXX011b
                                int 6
                        choice "Interrupt Request IRQ7"
                                pos[3]=XXXXX100b
                                int 7
                        choice "Interrupt Request IRQ12"
                                pos[3]=XXXXX101b
                                int 12
                        choice "Interrupt Request IRQ14"
                                pos[3]=XXXXX110b
                                int 14
                        choice "Interrputs Disabled"
                                pos[3]=XXXXX111b
                help
                        "Normally, the default setting of IRQ2 is satisfactory for
the interrupt level request. Reference the Owner's Guide for more details regarding
choosing an interrupt level. Be sure to make note of the interrupt level selected
for the network shell installation. Warning! Do not attempt to access the network with
the interrupts disabled."

        nameditem
                prompt "Extended Timeout Select"
                        choice "Response Time = 74.7 us"
                                pos[1]=11XXXXXXb
                        choice "Response Time = 283.4 us"
                                pos[1]=10XXXXXXb
                        choice "Response Time = 561.8 us"
                                pos[1]=01XXXXXXb
                        choice "Response Time = 1118.6 us"
                                pos[1]=00XXXXXXb
                help
                        "To configure this adapter, the network extended timeout must be
selected. Under ordinary circumstances, select a 74.7 us response time. Warning!
All nodes must be configured with the same network response time. See the Owner's Guide
for more details."

        nameditem
                prompt "Boot PROM Base Address Select"
                        choice "PROM Disabled"
                                pos[1]=XX00XXXb
                        choice "Offset 0C000"
                                pos[0]=0000XXXXb
                                pos[1]=XX01XXXb
                                mem 0C0000h-0C07FFh
                        choice "Offset 0C200"
                                pos[0]=0001XXXXb
                                pos[1]=XX01XXXb
                                mem 0C2000h-0C27FFh
                        choice "Offset 0C400"
                                pos[0]=0010XXXXb
                                pos[1]=XX01XXXb
                                mem 0C4000h-0C47FFh
                        choice "Offset 0C600"
                                pos[0]=0011XXXXb
                                pos[1]=XX01XXXb
                                mem 0C6000h-0C7FFFh
                        choice "Offset 0C800"
                                pos[0]=0100XXXXb
                                pos[1]=XX01XXXb
                                mem 0C8000h-0C87FFh
                        choice "Offset 0CA00"
                                pos[0]=0101XXXXb
                                pos[1]=XX01XXXb
                                mem 0CA000h-0CA7FFh
                        choice "Offset 0CC00"
                                pos[0]=0110XXXXb
                                pos[1]=XX01XXXb
                                mem 0CC000h-0CC7FFh
                        choice "Offset 0CE00"
                                pos[0]=0111XXXXb
                                pos[1]=XX01XXXb
                                mem 0CE000h-0CE7FFh
                        choice "Offset 0D000"
                                pos[0]=1000XXXXb
                                pos[1]=XX01XXXb
                                mem 0D0000h-0D07FFh
                        choice "Offset 0D200"
                                pos[0]=1001XXXXb
                                pos[1]=XX01XXXb
                                mem 0D2000h-0D27FFh
                        choice "Offset 0D400"
                                pos[0]=1010XXXXb
                                pos[1]=XX01XXXb
                                mem 0D4000h-0D47FFh
                        choice "Offset 0D600"
                                pos[0]=1011XXXXb
                                pos[1]=XX01XXXb
                                mem 0D6000h-0D7FFFh
                        choice "Offset 0D800"
                                pos[0]=1100XXXXb
                                pos[1]=XX01XXXb
                                mem 0D8000h-0D87FFh
                        choice "Offset 0DA00"
                                pos[0]=1101XXXXb
                                pos[1]=XX01XXXb
                                mem 0DA000h-0DA7FFh
                        choice "Offset 0DC00"
                                pos[0]=1110XXXXb
                                pos[1]=XX01XXXb
                                mem 0DC000h-0DC7FFh
                        choice "Offset 0DE00"
                                pos[0]=1111XXXXb
                                pos[1]=XX01XXXb
                                mem 0DE000h-0DE7FFh
                help
                        "In order to perform a diskless boot, the adapter board must have
a boot PROM and a nonconflicting offset address between 0C000-0DE00 must be selected. A 
conflict condition is indicated with an asterisk (*) at end of the base address offset 
selected. Choose <PROM DISABLED> if there isn't a boot PROM on the board or to remove the 
PROM from the computer's address space."