AdapterId  06A14h  						

AdapterName  "NCR WaveLAN  Adapter"    			

NumBytes  4 

NamedItem

Prompt  "I/O Address Range :"					

Choice  "0400h-O7FFh"  pos[3]= xx000001b  io 0400h-07FFh
Choice  "0800h-0BFFh"  pos[3]= xx000010b  io 0800h-0BFFh
Choice  "0C00h-0FFFh"  pos[3]= xx000011b  io 0C00h-0FFFh
Choice  "1000h-13FFh"  pos[3]= xx000100b  io 1000h-13FFh
Choice  "1400h-17FFh"  pos[3]= xx000101b  io 1400h-17FFh
Choice  "1800h-1BFFh"  pos[3]= xx000110b  io 1800h-1BFFh
Choice  "1C00h-1FFFh"  pos[3]= xx000111b  io 1C00h-1FFFh
Choice  "2000h-23FFh"  pos[3]= xx001000b  io 2000h-23FFh
Choice  "2400h-27FFh"  pos[3]= xx001001b  io 2400h-27FFh
Choice  "2800h-2BFFh"  pos[3]= xx001010b  io 2800h-2BFFh
Choice  "2C00h-2FFFh"  pos[3]= xx001011b  io 2C00h-2FFFh
Choice  "3000h-33FFh"  pos[3]= xx001100b  io 3000h-33FFh
Choice  "3400h-37FFh"  pos[3]= xx001101b  io 3400h-37FFh
Choice  "3800h-3BFFh"  pos[3]= xx001110b  io 3800h-3BFFh
Choice  "3C00h-3FFFh"  pos[3]= xx001111b  io 3C00h-3FFFh
Choice  "4000h-43FFh"  pos[3]= xx010000b  io 4000h-43FFh


Help

"16 possible I/O addresses are supported by the WaveLAN adapter.
Use the F5=Previous and the F6=Next to change this assignment.
Conflicting assignments are marked with an asterisk and must be changed."

NamedItem

Prompt  "ROM Address Range :"

Choice  "No ROM present "  pos[0]= xxx1111xb 
Choice  "0C0000h-0C3FFFh"  pos[0]= xxx0000xb  MEM 0C0000h-0C3FFFh
Choice  "0C4000h-0C7FFFh"  pos[0]= xxx0010xb  MEM 0C4000h-0C7FFFh
Choice  "0C8000h-0CBFFFh"  pos[0]= xxx0100xb  MEM 0C8000h-0CBFFFh
Choice  "0CC000h-0CFFFFh"  pos[0]= xxx0110xb  MEM 0CC000h-0CFFFFh
Choice  "0D0000h-0D3FFFh"  pos[0]= xxx1000xb  MEM 0D0000h-0D3FFFh
Choice  "0D4000h-0D7FFFh"  pos[0]= xxx1010xb  MEM 0D4000h-0D7FFFh
Choice  "0D8000h-0DBFFFh"  pos[0]= xxx1100xb  MEM 0D8000h-0DBFFFh
Choice  "0DC000h-0DFFFFh"  pos[0]= xxx1110xb  MEM 0DC000h-0DFFFFh

Help

" The first choice disables the adapter for Remote Boot Operation via the LAN.
The other choices correspond to 8 possible ROM address ranges for Remote Boot
Operation which are supported by the WaveLAN adapter.
Use the F5=Previous and the F6=Next to change this assignment.
Conflicting assignments are marked with an asterisk and must be changed."

NamedItem

Prompt  "Interrupt Select :"

Choice  "Interrupt 10 (Highest priority)"  pos[1]= xxxxx000b INT 10
Choice  "Interrupt 11                   "  pos[1]= xxxxx001b INT 11
Choice  "Interrupt 12                   "  pos[1]= xxxxx010b INT 12
Choice  "Interrupt 15                   "  pos[1]= xxxxx011b INT 15
Choice  "Interrupt  3                   "  pos[1]= xxxxx100b INT  3
Choice  "Interrupt  5 (Lowest priority) "  pos[1]= xxxxx101b INT  5


Help

"1 out of 6 possible interrupts can be assigned to the WaveLAN adapter.
Use the F5=Previous and the F6=Next to change this assignment.
The selected Interrupt must be unique for the WaveLAN Adapter Card."


