
AdapterId 05126h

AdapterName "Tecmar Floppy Tape Controller"   

NumBytes 2

NamedItem
        Prompt "Floppy Tape Controller I/O Location"
      choice "I/O 300"    pos[0]=XXXX000Xb  io 0300h-0307h
      choice "I/O 310"    pos[0]=XXXX100Xb  io 0310h-0317h
      choice "I/O 320"    pos[0]=XXXX010Xb  io 0320h-0327h
      choice "I/O 330"    pos[0]=XXXX110Xb  io 0330h-0337h
      choice "I/O 340"    pos[0]=XXXX001Xb  io 0340h-0347h
      choice "I/O 350"    pos[0]=XXXX101Xb  io 0350h-0357h
      choice "I/O 360"    pos[0]=XXXX011Xb  io 0360h-0367h
      choice "I/O 370"    pos[0]=XXXX111Xb  io 0370h-0377h

   Help
 "This port can be assigned to any of eight (8) I/O locations. 
 Use the F5=Previous and the F6=Next keys to change this
 assignment in the 'Change configuration' window.  Conflicting
 assignments are marked with an asterisk and must be changed to
 use the adapter."

NamedItem
        Prompt "Floppy Tape Controller Interrupt Number"
      choice "Int  3"   pos[0]=XX00XXXXb  int  3
      choice "Int  4"   pos[0]=XX10XXXXb  int  4
      choice "Int  5"   pos[0]=XX01XXXXb  int  5
      choice "Int  6"   pos[0]=XX11XXXXb  int  6
			     
   Help
      "This assignment need only be changed if you do not wish certain
      programs to share interrupts. Use the F5=Previous and the F6=Next keys
      to change arbitration level assignments if you are in the
      'Change configuration' window."

NamedItem
        Prompt "Floppy Tape Controller DMA Arbitration"
      choice "Level 1"   pos[1]=XXXX0001b  arb  1
      choice "Level 2"   pos[1]=XXXX0010b  arb  2
      choice "Level 3"   pos[1]=XXXX0011b  arb  3
      choice "Level 5"   pos[1]=XXXX0101b  arb  5
      choice "Level 6"   pos[1]=XXXX0110b  arb  6
      choice "Level 7"   pos[1]=XXXX0111b  arb  7
      choice "Level 0"   pos[1]=XXXX0000b  arb  0
      choice "Level 4"   pos[1]=XXXX0100b  arb  4


  Help
      "This assignment need only be changed if it is in conflict
      with another assignment.  Conflicting assignments are marked
      with an asterisk.  Use the F5=Previous and the F6=Next keys
      to change arbitration level assignments if you are in the
      'Change configuration' window."
