; 
;	$Revision:   1.3  $
;	$Date:   09 Dec 1991 15:12:10  $
; 
;***************************************************************************
;* Copyright (C) 1988 by Phoenix Technologies Ltd.  			   *
;* Copyright (C) 1989 by NCR Corporation    This program		   *
;* contains proprietary and confidential information.  All rights reserved *
;* except as may be permitted by prior written consent.                    *
;*************************************************************************** 
; SYS0200.ADF

; If the configuration file does NOT have the NOWAITF1 flag then this file
; will be parsed in and displayed.

; Let SETUP know this will require a valid CMOS signature to have effect
PSignature

;******************************************************************
; CMOS 701 - POST F1 key control
;   bit 0 = Diskette error.
;           1 - Do not wait for F1 key
;           0 - Wait for F1 key
;   bit 1 = CRT (video) error.
;           1 - Do not wait for F1 key
;           0 - Wait for F1 key
;   bit 2 = keyboard error. (Note the bit-definition is reversed)
;           1 - Wait for F1 key
;           0 - Do not wait for F1 key
;******************************************************************
NamedItem			  
	ECmos 701h
	Prompt "POST Waits for F1 on Diskette Errors"
	Choice "Yes" pos[0]=XXXXXXX0b
	Choice "No"  pos[0]=XXXXXXX1b
	Help
" If POST finds a diskette error (601 or 602) it will optionally wait 
for the user to acknowledge the error by pressing the F1 key. If this 
feature set to Yes then POST will wait for for the F1 key. If its set 
to No then POST will not wait for F1 key."

nameditem
	ECmos 701h
	Prompt "POST Waits for F1 on Video Errors"
	Choice "Yes" pos[0]=XXXXXX0Xb
	Choice "No"  pos[0]=XXXXXX1Xb
	Help
" If POST finds a video controller error (2401) it will optionally wait
for the user to acknowledge the error by pressing the F1 key. If this 
feature set to Yes then POST will wait for for the F1 key. If its set to 
No then POST will not wait for F1 key."

nameditem
	ECmos 701h
	Prompt "POST Waits for F1 on Keyboard Errors"
	Choice "Yes" pos[0]=XXXXX1XXb
	Choice "No"  pos[0]=XXXXX0XXb
	Help 
" If POST finds a keyboard error (301, 304, 306 or 307) it will 
optionally wait for the user to	acknowledge the error by pressing 
the F1 key. If this feature set to Yes then POST will wait for for 
the F1 key. If its set to No then POST will not wait for F1 key."
