;***********************************************************   
;
;       Cornerstone Technology, Inc.            
;       06/21/91
;
;***********************************************************   
AdapterId 080A5h
AdapterName "High Resolution Display"             
NumBytes 4

NamedItem       Prompt  "I/O base address"
	choice "1000" pos[1]=XXXXX000b  io 1000h-100Fh
	choice "1010" pos[1]=XXXXX001b  io 1010h-101Fh
	choice "2000" pos[1]=XXXXX010b  io 2000h-200Fh
	choice "2010" pos[1]=XXXXX011b  io 2010h-201Fh
	choice "3000" pos[1]=XXXXX100b  io 3000h-300Fh
	choice "3010" pos[1]=XXXXX101b  io 3010h-301Fh
	choice "4000" pos[1]=XXXXX110b  io 4000h-400Fh
	choice "4010" pos[1]=XXXXX111b  io 4010h-401Fh
Help
"Choose a block with no conflicts."

NamedItem       Prompt  "RAM base segment address"
	choice "0C8000"     pos[1]=XX000XXXb  mem 0C8000h-0CFFFFh
	choice "0D0000"     pos[1]=XX001XXXb  mem 0D0000h-0D7FFFh
	choice "0D8000"     pos[1]=XX010XXXb  mem 0D8000h-0DFFFFh
Help
"Choose a block with no conflicts."

NamedItem       Prompt  "ROM base segment address"
	choice "0C0000"     pos[2]=XXXXX000b  mem 0C0000h-0C1FFFh
	choice "0C2000"     pos[2]=XXXXX001b  mem 0C2000h-0C3FFFh
	choice "0C4000"     pos[2]=XXXXX010b  mem 0C4000h-0C5FFFh
	choice "0C6000"     pos[2]=XXXXX100b  mem 0C6000h-0C7FFFh
Help
"Choose a block with no conflicts."

NamedItem       Prompt  "Invert FG clock"
	choice "Standard FG clock" pos[2]=XXXX0XXXb        
	choice "Inverted FG clock" pos[2]=XXXX1XXXb
Help
"This option is not used for the DualPage 120.
Inverted FG clock is required for the DualPage and SinglePage XL for IBM PS/2 model 50 and Bull computers.
Try changing this setting if the edges of displayed characters appear unstable."

NamedItem       Prompt  "Default Video Device"
	choice "High Resolution Monitor" pos[1]=00XXXXXXb pos[3]=XXXXXXX1b        
	choice "VGA Monitor" pos[1]=10XXXXXXb pos[3]=XXXXXXX1b
Help
"Select primary video output device."
