
AdapterID 08DF3h

AdapterName "DSS and sub card 3"

Numbytes 2

FixedResources
        pos[1]=0xxxxxxxb
        pos[0]=00xxxxx1b
;       mem 0D0000h-0D3FFFh
;       io 1D00h-1D7Fh

Nameditem
        Prompt  "DMA Arbitration Level"
          Choice  "Level 5"
             POS[0]=xxx0101xb
             arb 5
          Choice  "Level 6"
             POS[0]=xxx0110xb
             arb 6
          Choice  "Level 7"
             POS[0]=xxx0111xb
             arb 7
          Choice  "Level 8"
             POS[0]=xxx1000xb
             arb 8
          Choice  "Level 9"
             POS[0]=xxx1001xb
             arb 9
          Choice  "Level 10"
             POS[0]=xxx1010xb
             arb 10
          Choice  "Level 11"
             POS[0]=xxx1011xb
             arb 11
          Choice  "Level 12"
             POS[0]=xxx1100xb
             arb 12
          Choice  "Level 13"
             POS[0]=xxx1101xb
             arb 13
          Choice  "Level 14"
             POS[0]=xxx1110xb
             arb 14
          Choice  "Level 15"
             POS[0]=xxx1111xb
             arb 15
          Choice  "Level 0"
             POS[0]=xxx0000xb
             arb 0
          Choice  "Level 1"
             POS[0]=xxx0001xb
             arb 1
          Choice  "Level 2"
             POS[0]=xxx0010xb
             arb 2
        Choice  "Level 3"
             POS[0]=xxx0011xb
             arb 3
        Choice  "Level 4"
             POS[0]=xxx0100xb
             arb 4
        Help
        "This selects the DMA channel arbitration level that the adapter
        will use.
        Under normal circumstances, select 5, this is an arbitary
        decision!"

nameditem
        Prompt  "Fairness On/Off"
        Choice  "On"
             POS[0]=xx1xxxxxb
        Choice  "Off"
             POS[0]=xx0xxxxxb
        Help
        "Bus Arbitration Fairness.  This controls whether the adapter
        will release control of the bus when it has been using it
        exclusively.  Under normal circumstances select ON."

Nameditem
        Prompt  "Adapter I/O Addressing"
        Choice  "I/O Addresses 1D00 to 1D7F"
             POS[1]=xxxxxx00b
             io 1D00h-1D7Fh
        Choice  "I/O Addresses 2D00 to 2D7F"
             POS[1]=xxxxxx01b
             io 2D00h-2D7Fh
        Choice  "I/O Addresses 3D00 to 3D7F"
             POS[1]=xxxxxx10b
             io 3D00h-3D7Fh
        Choice  "I/O Addresses 4D00 to 4D7F"
             POS[1]=xxxxxx11b
             io 4D00h-4D7Fh
        Help
        "This determines Adapter I/O Addressing locations."

nameditem
       Prompt  "Adapter Memory Location"
       Choice  "Segment C0000"
            POS[1]=x00000xxb
            MEM  0C0000h-0C1FFFh
       Choice  "Segment C2000"
            POS[1]=x00010xxb
            MEM  0C2000h-0C3FFFh
       Choice  "Segment C4000"
            POS[1]=x00100xxb
            MEM  0C4000h-0C5FFFh
       Choice  "Segment C6000"
            POS[1]=x00110xxb
            MEM  0C6000h-0C7FFFh
       Choice  "Segment C8000"
            POS[1]=x01000xxb
            MEM  0C8000h-0C9FFFh
       Choice  "Segment CA000"
            POS[1]=x01010xxb
            MEM  0CA000h-0CBFFFh
       Choice  "Segment CC000"
            POS[1]=x01100xxb
            MEM  0CC000h-0CDFFFh
       Choice  "Segment CE000"
            POS[1]=x01010xxb
            MEM  0CE000h-0CFFFFh
       Choice  "Segment D0000"
            POS[1]=x10000xxb
            MEM  0D0000h-0D1FFFh
       Choice  "Segment D2000"
            POS[1]=x10010xxb
            MEM  0D2000h-0D3FFFh
       Choice  "Segment D4000"
            POS[1]=x10100xxb
            MEM  0D4000h-0D5FFFh
       Choice  "Segment D6000"
            POS[1]=x10110xxb
            MEM  0D6000h-0D7FFFh
       Choice  "Segment D8000"
            POS[1]=x11000xxb
            MEM  0D8000h-0D9FFFh
       Choice  "Segment DA000"
            POS[1]=x11010xxb
            MEM  0DA000h-0DBFFFh
       Choice  "Segment DC000"
            POS[1]=x11100xxb
            MEM  0DC000h-0DDFFFh
       Choice  "Segment DE000"
            POS[1]=x11110xxb
            MEM  0DE000h-0DFFFFh
       Choice  "ROM Disable"
            POS[1]=x00001xxb
       Help
       "To configure this adapter you must choose the memory location
        the adapter will use for the BIOS ROM, and RAM window.  There
        are sixteen memory locations that can be selected.    Under
        normal circumstances a video adapter will select location
        C0000."
