AdapterId 00F7Fh

AdapterName "PSconnect"

NumBytes 8

FixedResources
 pos[0]=10100101b
 pos[3]=01x0xxxxb

NamedItem
Prompt "FIFO R/W port address"
 choice "Port_200"
      pos[1]=xxxx0000b
      io 0200h-0207h 
 choice "Port_210"
      pos[1]=xxxx0001b
      io 0210h-0217h 
 choice "Port_300"
      pos[1]=xxxx0010b
      io 0300h-0307h 
 choice "Port_310"
      pos[1]=xxxx0011b
      io 0310h-0317h 
 choice "Port_1200"
      pos[1]=xxxx0100b
      io 01200h-01207h 
 choice "Port_1210"
      pos[1]=xxxx0101b
      io 01210h-01217h 
 choice "Port_1300"
      pos[1]=xxxx0110b
      io 01300h-01307h 
 choice "Port_1310"
      pos[1]=xxxx0111b
      io 01310h-01317h 
 choice "Port_2200"
      pos[1]=xxxx1000b
      io 02200h-02207h 
 choice "Port_2210"
      pos[1]=xxxx1001b
      io 02210h-02217h 
 choice "Port_2300"
      pos[1]=xxxx1010b
      io 02300h-02307h 
 choice "Port_2310"
      pos[1]=xxxx1011b
      io 02310h-02317h 
 choice "Port_3200"
      pos[1]=xxxx1100b
      io 03200h-03207h 
 choice "Port_3210"
      pos[1]=xxxx1101b
      io 03210h-03217h 
 choice "Port_3300"
      pos[1]=xxxx1110b
      io 03300h-03307h 
 choice "Port_3310"
      pos[1]=xxxx1111b
      io 03310h-03317h 
 Help
"Select the desired port address for the R/W FIFO.
Use the F5=Previous and F6=Next keys to change the selection."

NamedItem
Prompt "Reset write/FIFO status read port address"
 choice "Port_208"
      pos[1]=0000xxxxb
      io 0208h-020fh
 choice "Port_218"
      pos[1]=0001xxxxb
      io 0218h-021fh
 choice "Port_308"
      pos[1]=0010xxxxb
      io 0308h-030fh
 choice "Port_318"
      pos[1]=0011xxxxb
      io 0318h-031fh
 choice "Port_1208"
      pos[1]=0100xxxxb
      io 01208h-0120fh
 choice "Port_1218"
      pos[1]=0101xxxxb
      io 01218h-0121fh
 choice "Port_1308"
      pos[1]=0110xxxxb
      io 01308h-0130fh
 choice "Port_1318"
      pos[1]=0111xxxxb
      io 01318h-0131fh
 choice "Port_2208"
      pos[1]=1000xxxxb
      irompt "CROM shadow CC000 - CDFFFH"
	Choice "Disable"	pos[0]=X1XXXXXXb
	Choice "Enable"		pos[0]=X0XXXXXXb
	Help
"Forces shadowing of Channel ROM in the given memory range."
; ***********************************************************
NamedItem
	ECMOS 950h
	Prompt "CROM shadow CE000 - CFFFFH"
	Choice "Disable"	pos[0]=1XXXXXXXb
	Choice "Enable"		pos[0]=0XXXXXXXb
	Help
"Forces shadowing of Channel ROM in the given memory range."
; ***********************************************************

; ***********************************************************
NamedItem
	ECMOS 951h
	Prompt "CROM shadow D0000 - D1FFFH"
	Choice "Disable"	pos[0]=XXXXXXX1b
	Choice "Enable"		pos[0]=XXXXXXX0b
	Help
"Forces shadowing of Channel ROM in the given memory range."
; ***********************************************************

NamedItem
	ECMOS 951h
	Prompt "CROM shadow D2000 - D3FFFH"
	Choice "Disable"	pos[0]=XXXXXX1Xb
	Choice "Enable"		pos[0]=XXXXXX0Xb
	Help
"Forces shadowing of Channel ROM in the given memory range."
; ***********************************************************
NamedItem
	ECMOS 951h
	Prompt "CROM shadow D4000 - D5FFFH"
	Choice "Disable"	pos[0]=XXXXX1XXb
	Choice "Enable"		pos[0]=XXXXX0XXb
	Help
"Forces shadowing of Channel ROM in the given memory range."
; ***********************************************************
NamedItem
	ECMOS 951h
	Prompt "CROM shadow D6000 - D7FFFH"
	Choice "Disable"	pos[0]=XXXX1XXXb
	Choice "Enable"		pos[0]=XXXX0XXXb
	Help
"Forces shadowing of Channel ROM in the given memory range."
; ***********************************************************
NamedItem
	ECMOS 951h
	Prompt "CROM shadow D8000 - D9FFFH"
	Choice "Disable"	pos[0]=XXX1XXXXb
	Choice "Enable"		pos[0]=XXX0XXXXb
	Help
"Forces shadowing of Channel ROM in the given memory range."
; ***********************************************************
NamedItem
	ECMOS 951h
	Prompt "CROM shadow DA000 - DBFFFH"
	Choice "Disable"	pos[0]=XX1XXXXXb
	Choice "Enable"		pos[0]=XX0XXXXXb
	Help
"Forces shadowing of Channel ROM in the given memory range."
; ***********************************************************
NamedItem
	ECMOS 951h
	Prompt "CROM shadow DC000 - DDFFFH"
	Choice "Disable"	pos[0]=X1XXXXXXb
	Choice "Enable"		pos[0]=X0XXXXXXb
	Help
"Forces shadowing of Channel ROM in the given memory range."
; ***********************************************************
NamedItem
	ECMOS 951h
	Prompt "CROM shadow DE000 - DFFFFH"
	Choice "Disable"	pos[0]=1XXXXXXXb
	Choice "Enable"		pos[0]=0Xange arbitration levels.
Level 0 has the highest priority, level 7 the lowest."
