AdapterID 06AE0h

AdapterName  "SCSI Fixed Disk Controller"

NumBytes 4

fixedresources
        pos[2]=00000000b
        int 14

nameditem
        Prompt  "Adapter I/O Location"
          Choice "Adr I/O 400h"
            pos[1]=01000000b
            io 0400h-040fh
          Choice "Adr I/O 500h"
            pos[1]=01010000b
            io 0500h-050fh
          Choice "Adr I/O 600h"
            pos[1]=01100000b
            io 0600h-060fh
          Choice "Adr I/O 700h"
            pos[1]=01110000b
            io 0700h-070fh
          Choice "Adr I/O 800h"
            pos[1]=10000000b
            io 0800h-080fh
          Choice "Adr I/O 900h"
            pos[1]=10010000b
            io 0900h-090fh
        Help
        "To configure this adapter you must choose the I/O location the
         adapter will use . Under normal circumstances, select < Adr I/O 400h>."

nameditem
        Prompt  "DMA Arbitration Level"
          Choice  "Level 3"
            pos[0]=XXX0011Xb
            arb 3
          Choice  "Level 4"
            pos[0]=XXX0100Xb
            arb 4
          Choice  "Level 0"
            pos[0]=XXX0000Xb
            arb 0
          Choice  "Level 1"
            pos[0]=XXX0001Xb
            arb 1
          Choice  "Level 5"
            pos[0]=XXX0101Xb
            arb 5
          Choice  "Level 6"
            pos[0]=XXX0110Xb
            arb 6
          Choice  "Level 7"
            pos[0]=XXX0111Xb
            arb 7
          Choice  " No DMA "
            pos[0]=XXX1111Xb
        Help
        "This selects the DMA channel the adapter will use to transfer data.
         Under normal circumstances, select option <Level 3> ...
         WARNING : The option <No DMA> means Programmed I/O in Burst mode
         and depends on the HARDWARE : (SCSI disk capability transfer rate and CPU speed),
         DESTRUCTIVE errors may appear if this selection is not appropriate !!"

nameditem
        Prompt  "Fairness On/Off"
          Choice  "On"
            pos[3]=XXX0XXXXb
          Choice  "Off"
            pos[3]=XXX1XXXXb
        Help
        "Bus Arbitration Fairness.  This controls whether the adapter will
         release control of the bus when it has been using it exclusively.
         Under normal circumstances, select <On>."
