;
;Note to translators:
;
;This file is used when doing the system configuration for the
;3363 Optical Drive Adapter cards.
;
;CAUTION:
;
;ONLY TRANSLATE THE LINES THAT ARE IN QUOTES ("------")
;NOTHING ELSE NEEDS TO BE CHANGED.
;
;The commented line just below the line in quotes remains unchanged.
;
;KEYWORDS just before or as a heading or contained in the line are
;not to be translated only that part of the line in quotes, ("-----").
;Example:
;         choice  "Address 258" pos[0]=XXXX000Xb io 0258h-025Bh
;Only the "Address 258" is to be translated, all else remains as is.
;
;KEYWORDS ARE:  Adapter ID, AdapterName, NumBytes, fixedresources,
;nameditem, Prompt, Help, choice or Choice, pos, io, mem, int, and arb.
;
;Each Section of selections is repeated as a total section along with
;its help section therefore, the unchanged part is repeated just below
;the section to be translated.  Doing it in this manner will make
;it easier to read.
;
;Paragraph statements, such as those under the  Help (Keyword) are
;written as a total statement between its set of quote marks.  Each
;unchanged help statemnet is repeated below the section that it
;refers to.

AdapterID 0DF7Fh

AdapterName  "IBM3363 Optical Disk"
;AdapterName  IBM3363 Optical Disk

NumBytes 4

fixedresources
	pos[0]=XXXXXXXXb
	pos[1]=XXXXXXXXb
	pos[2]=XXXXXXXXb
	pos[3]=XXXXXXXXb

nameditem
	Prompt "IO Address Select"
	  choice  "Address 258" pos[0]=XXXX000Xb io 0258h-025Bh
	  choice  "Address 658" pos[0]=XXXX001Xb io 0658h-065Bh
	  choice  "Address A58" pos[0]=XXXX010Xb io 0a58h-0a5Bh
	  choice  "Address E58" pos[0]=XXXX011Xb io 0e58h-0e5Bh
	Help
	"Set up the port addresses for the card. Each optical
	 adapter must have a unique address range. Under normal
	 conditions, allow the default, otherwise step through
	 until you find an address which is not in conflict."

;	Prompt  IO Address Select
;	  choice   Address 258  pos[0]=XXXX000Xb io 0258h-025Bh
;	  choice   Address 658  pos[0]=XXXX001Xb io 0658h-065Bh
;	  choice   Address A58  pos[0]=XXXX010Xb io 0a58h-0a5Bh
;	  choice   Address E58  pos[0]=XXXX011Xb io 0e58h-0e5Bh
;	Help
;	 Set up the port addresses for the card. Each optical
;	 adapter must have a unique address range. Under normal
;	 conditions, allow the default, otherwise step through
;	 until you find an address which is not in conflict.

nameditem
	Prompt	"ROS Segment"
	  Choice "Segment DA00" pos[0]=1101XXXXb  mem 0DA000h-0DBFFFh
	  Choice "Segment DC00" pos[0]=1110XXXXb  mem 0DC000h-0DDFFFh
	  Choice "Segment DE00" pos[0]=1111XXXXb  mem 0DE000h-0DFFFFh
	  Choice "Segment C800" pos[0]=0100XXXXb  mem 0C8000h-0C9FFFh
	  Choice "Segment CA00" pos[0]=0101XXXXb  mem 0CA000h-0CBFFFh
	  Choice "Segment CC00" pos[0]=0110XXXXb  mem 0CC000h-0CDFFFh
	  Choice "Segment CE00" pos[0]=0111XXXXb  mem 0CE000h-0CFFFFh
	  Choice "Segment D000" pos[0]=1000XXXXb  mem 0D0000h-0D1FFFh
	  Choice "Segment D200" pos[0]=1001XXXXb  mem 0D2000h-0D3FFFh
	  Choice "Segment D400" pos[0]=1010XXXXb  mem 0D4000h-0D5FFFh
	  Choice "Segment D600" pos[0]=1011XXXXb  mem 0D6000h-0D7FFFh
	  Choice "Segment D800" pos[0]=1100XXXXb  mem 0D8000h-0D9FFFh
	Help
	"To configure this adapter you must choose the memory location the
	 adapter will use for it's BIOS ROM.  There are 12 memory locations
	 that can be selected.	Under normal circumstances, select the
	 default, otherwise step through until you find an address which
	 is not in conflict."

;	Prompt	 ROS Segment
;	  Choice  Segment DA00  pos[0]=1101XXXXb  mem 0DA000h-0DBFFFh
;	  Choice  Segment DC00  pos[0]=1110XXXXb  mem 0DC000h-0DDFFFh
;	  Choice  Segment DE00  pos[0]=1111XXXXb  mem 0DE000h-0DFFFFh
;	  Choice  Segment C800  pos[0]=0100XXXXb  mem 0C8000h-0C9FFFh
; 	  Choice  Segment CA00  pos[0]=0101XXXXb  mem 0CA000h-0CBFFFh
;	  Choice  Segment CC00  pos[0]=0110XXXXb  mem 0CC000h-0CDFFFh
;	  Choice  Segment CE00  pos[0]=0111XXXXb  mem 0CE000h-0CFFFFh
;	  Choice  Segment D000  pos[0]=1000XXXXb  mem 0D0000h-0D1FFFh
;	  Choice  Segment D200  pos[0]=1001XXXXb  mem 0D2000h-0D3FFFh
;	  Choice  Segment D400  pos[0]=1010XXXXb  mem 0D4000h-0D5FFFh
;	  Choice  Segment D600  pos[0]=1011XXXXb  mem 0D6000h-0D7FFFh
;	  Choice  Segment D800  pos[0]=1100XXXXb  mem 0D8000h-0D9FFFh
;	Help
;	 To configure this adapter you must choose the memory location the
;	 adapter will use for it's BIOS ROM.  There are 12 memory locations
;	 that can be selected.	Under normal circumstances, select the
;	 default, otherwise step through until you find an address which
;	 is not in conflict.

nameditem
	Prompt "PIO/DMA IO"
	  choice  "DMA Data Transfer" pos[1]=1XXXXXXXb
	  choice  "PIO Data Transfer" pos[1]=0XXXXXXXb
	Help
	"This adapter can transfer data via PIO or DMA.
	Under normal conditions allow the default to DMA.
	Step through arbitration levels until you find a
	level which is not in conflict."

;	Prompt  PIO/DMA IO
;	  choice   DMA Data Transfer  pos[1]=1XXXXXXXb
;	  choice   PIO Data Transfer  pos[1]=0XXXXXXXb
;	Help
;	 This adapter can transfer data via PIO or DMA.
;	Under normal conditions allow the default to DMA.
;	Step through arbitration levels until you find a
;	level which is not in conflict.

nameditem
	Prompt	"Interrupt Level"
	  Choice  "5"  pos[1]=X00XXXXXb int 5
	  Choice  "7"  pos[1]=X01XXXXXb int 7
	  Choice  "10" pos[1]=X10XXXXXb int 10
	  Choice  "11" pos[1]=X11XXXXXb int 11
	Help
	"This adapter can use any of four interrupt levels.
	Under normal conditions allow the default."

;	Prompt	 Interrupt Level
;	  Choice   5   pos[1]=X00XXXXXb int 5
;	  Choice   7   pos[1]=X01XXXXXb int 7
;	  Choice   10  pos[1]=X10XXXXXb int 10
;	  Choice   11  pos[1]=X11XXXXXb int 11
;	Help
;	 This adapter can use any of four interrupt levels.
;	Under normal conditions allow the default.

nameditem
	Prompt	"Fairness On/Off"
	  Choice  "On"  pos[1]=XXX1XXXXb
	  Choice  "Off" pos[1]=XXX0XXXXb
	Help
	"Bus Arbitration Fairness.  This controls whether the adapter will
	 release control of the bus when it has been using it exclusively.
	 Under normal circumstances, select <On>."

;	Prompt	 Fairness On/Off
;	  Choice   On   pos[1]=XXX1XXXXb
;	  Choice   Off  pos[1]=XXX0XXXXb
;	Help
;	 Bus Arbitration Fairness.  This controls whether the adapter will
;	 release control of the bus when it has been using it exclusively.
;	 Under normal circumstances, select <On>.

nameditem
	Prompt	"Arbitration Level"
	  Choice  "Level 10" pos[1]=XXXX1010b arb 10
	  Choice  "Level 11" pos[1]=XXXX1011b arb 11
	  Choice  "Level 12" pos[1]=XXXX1100b arb 12
	  Choice  "Level 13" pos[1]=XXXX1101b arb 13
	  Choice  "Level 14" pos[1]=XXXX1110b arb 14
	  Choice  "Level  0" pos[1]=XXXX0000b arb  0
	  Choice  "Level  1" pos[1]=XXXX0001b arb  1
	  Choice  "Level  2" pos[1]=XXXX0010b arb  2
	  Choice  "Level  3" pos[1]=XXXX0011b arb  3
	  Choice  "Level  4" pos[1]=XXXX0100b arb  4
	  Choice  "Level  5" pos[1]=XXXX0101b arb  5
	  Choice  "Level  6" pos[1]=XXXX0110b arb  6
	  Choice  "Level  7" pos[1]=XXXX0111b arb  7
	  Choice  "Level  8" pos[1]=XXXX1000b arb  8
	  Choice  "Level  9" pos[1]=XXXX1001b arb  9
	Help
	"This assignment need only be changed if it is in conflict
	with another assignment.  Conflicting assignments are marked
	with an asterisk.  Use the F5=Previous and the F6=Next keys
	to change arbitration level assignments.  Using arbitration
	levels, this adapter accesses memory directly without
	burdening the computer's main microprocessor.  An
	arbitration level of 0 has the highest priority, and
	increasing levels have corresponding decreased priority."

;	Prompt	 Arbitration Level
;	  Choice   Level 10  pos[1]=XXXX1010b arb 10
;	  Choice   Level 11  pos[1]=XXXX1011b arb 11
;	  Choice   Level 12  pos[1]=XXXX1100b arb 12
;	  Choice   Level 13  pos[1]=XXXX1101b arb 13
;	  Choice   Level 14  pos[1]=XXXX1110b arb 14
;	  Choice   Level  0  pos[1]=XXXX0000b arb  0
;	  Choice   Level  1  pos[1]=XXXX0001b arb  1
;	  Choice   Level  2  pos[1]=XXXX0010b arb  2
;	  Choice   Level  3  pos[1]=XXXX0011b arb  3
;	  Choice   Level  4  pos[1]=XXXX0100b arb  4
;	  Choice   Level  5  pos[1]=XXXX0101b arb  5
;	  Choice   Level  6  pos[1]=XXXX0110b arb  6
;	  Choice   Level  7  pos[1]=XXXX0111b arb  7
;	  Choice   Level  8  pos[1]=XXXX1000b arb  8
;	  Choice   Level  9  pos[1]=XXXX1001b arb  9
;	Help
;	 This assignment need only be changed if it is in conflict
;	with another assignment.  Conflicting assignments are marked
;	with an asterisk.  Use the F5=Previous and the F6=Next keys
;	to change arbitration level assignments.  Using arbitration
;	levels, this adapter accesses memory directly without
;	burdening the computer's main microprocessor.  An
;	arbitration level of 0 has the highest priority, and
;	increasing levels have corresponding decreased priority.

nameditem
	Prompt	"Burst Length"
	  Choice  "8  Byte Burst"   pos[2]=XXXX0111b
	  Choice  "7  Byte Burst"   pos[2]=XXXX0110b
	  Choice  "6  Byte Burst"   pos[2]=XXXX0101b
	  Choice  "5  Byte Burst"   pos[2]=XXXX0100b
	  Choice  "4  Byte Burst"   pos[2]=XXXX0011b
	  Choice  "3  Byte Burst"   pos[2]=XXXX0010b
	  Choice  "2  Byte Burst"   pos[2]=XXXX0001b
	  Choice  "Burst Disabled"  pos[2]=XXXX0000b
	Help
	"DMA transfer burst length.  This is the maximum number of bytes that
	 the adapter will transfer in a single DMA transfer.  Under normal
	 circumstances, select <8 Byte Burst>."

;	Prompt	 Burst Length
;	  Choice   8  Byte Burst    pos[2]=XXXX0111b
;	  Choice   7  Byte Burst    pos[2]=XXXX0110b
;	  Choice   6  Byte Burst    pos[2]=XXXX0101b
;	  Choice   5  Byte Burst    pos[2]=XXXX0100b
;	  Choice   4  Byte Burst    pos[2]=XXXX0011b
;	  Choice   3  Byte Burst    pos[2]=XXXX0010b
;	  Choice   2  Byte Burst    pos[2]=XXXX0001b
;	  Choice   Burst Disabled   pos[2]=XXXX0000b
;	Help
;	 DMA transfer burst length.  This is the maximum number of bytes that
;	 the adapter will transfer in a single DMA transfer.  Under normal
;	 circumstances, select <8 Byte Burst>.

nameditem
	Prompt "Bypass Diagnostics at REBOOT"
	  choice  "Run Diags"       pos[3]=1XXXXXX0b
	  choice  "Don't run diags" pos[3]=1XXXXXX1b
	Help
	"Diagnostics on the adapter card and drives are always
	 performed at power on time. This option selects a choice
	 of whether or not diagnostics are to be ran at REBOOT
	 time. <alt-ctrl-del>"

;	Prompt  Bypass Diagnostics at REBOOT
;	  choice   Run Diags        pos[3]=1XXXXXX0b
;	  choice   Don't run diags  pos[3]=1XXXXXX1b
;	Help
;	 Diagnostics on the adapter card and drives are always
;	 performed at power on time. This option selects a choice
;	 of whether or not diagnostics are to be ran at REBOOT
;	 time. <alt-ctrl-del>
