
AdapterID 08EFEh

AdapterName  "IBM PS/2 SCSI Adapter"

NumBytes 3

fixedresources
	pos[2]=1XxxxxxXb
	pos[1]=XXXXXXXXb
	pos[0]=xxxxXXXXb
	int 0eh exec

nameditem
	Prompt "I/O Address"
	  Choice  "3540-3547"
	    pos[0]=XXXX000Xb
	    io 3540h-3547h
	  Choice  "3548-354F"
	    pos[0]=XXXX001Xb
	    io 3548h-354Fh
	  Choice  "3550-3557"
	    pos[0]=XXXX010Xb
	    io 3550h-3557h
	  Choice  "3558-355F"
	    pos[0]=XXXX011Xb
	    io 3558h-355Fh
	  Choice  "3560-3567"
	    pos[0]=XXXX100Xb
	    io 3560h-3567h
	  Choice  "3568-356F"
	    pos[0]=XXXX101Xb
	    io 3568h-356Fh
	  Choice  "3570-3577"
	    pos[0]=XXXX110Xb
	    io 3570h-3577h
	  Choice  "3578-357F"
	    pos[0]=XXXX111Xb
	    io 3578h-357Fh
	Help
	 "This allows you to choose the I/O address for the adapter.
	 Each adapter must have a unique address range.  Under normal
	 circumstances, this address range does not need to be
	 changed.  Use the F5=Previous or the F6=Next keys to change
	 this assignment in the 'Change configuration' window.
	 Conflicting assignments are marked with an asterisk and must
	 be changed to use the adapter."

nameditem
	Prompt	"DMA Arbitration Level"
	  Choice  "Level C"
	    pos[1]=XXXX1100b
	    arb 0ch
	  Choice  "Level D"
	    pos[1]=XXXX1101b
	    arb 0dh
	  Choice  "Level E"
	    pos[1]=XXXX1110b
	    arb 0eh
	  Choice  "Level 1"
	    pos[1]=XXXX0001b
	    arb 1
	  Choice  "Level 3"
	    pos[1]=XXXX0011b
	    arb 3
	  Choice  "Level 5"
	    pos[1]=XXXX0101b
	    arb 5
	  Choice  "Level 6"
	    pos[1]=XXXX0110b
	    arb 6
	  Choice  "Level 7"
	    pos[1]=XXXX0111b
	    arb 7
	  Choice  "Level 8"
	    pos[1]=XXXX1000b
	    arb 8
	  Choice  "Level 9"
	    pos[1]=XXXX1001b
	    arb 9
	  Choice  "Level A"
	    pos[1]=XXXX1010b
	    arb 0ah
	  Choice  "Level B"
	    pos[1]=XXXX1011b
	    arb 0bh
	Help
	"This selects the DMA channel the adapter will use to transfer data.
	 Under normal circumstances, select <Level C>.	Use the F5=Previous
	 or the F6=Next keys to change this assignment in the 'Change
	 configuration' window."

nameditem
	Prompt	"Fairness On/Off"
	  Choice  "On"
	    pos[1]=XXX1XXXXb
	  Choice  "Off"
	    pos[1]=XXX0XXXXb
	Help
	"Bus Arbitration Fairness.  This controls whether the adapter will
	 release control of the bus when it has been using it exclusively.
	 Under normal circumstances, select <On>.  Use the F5=Previous or
	 the F6=Next keys to change this assignment in the 'Change
	 configuration' window."

nameditem
	Prompt	"ROM Wait State Disable"
	  Choice  "Enable Wait State"
	    pos[2]=XXXXXXX0b
	  Choice  "No Wait State"
	    pos[2]=XXXXXXX1b
	Help
	 "This allows you to set whether a wait state is added to
	 accesses of the ROM on the adapter.  Adapter performance
	 could be degraded if this is altered from the default.  Under
	 normal circumstances, select <Enable Wait State>.  Use the
	 F5=Previous or the F6=Next keys to change this assignment in
	 the 'Change configuration' window."

nameditem
	Prompt	"SCSI Adapter Address (ID)"
	  Choice "7"
	    pos[1]=111XXXXXb
	  Choice "6"
	    pos[1]=110XXXXXb
	  Choice "5"
	    pos[1]=101XXXXXb
	  Choice "4"
	    pos[1]=100XXXXXb
	  Choice "3"
	    pos[1]=011XXXXXb
	  Choice "2"
	    pos[1]=010XXXXXb
	  Choice "1"
	    pos[1]=001XXXXXb
	  Choice "0"
	    pos[1]=000XXXXXb
	Help
	"This allows you to change the SCSI ID of the adapter.
	 Under normal circumstances, select <7>.  Use the F5=Previous
	 or the F6=Next keys to change this assignment in the 'Change
	 configuration' window."
