
AdapterID 0FCCh

AdapterName  "D-Link Ethernet Card"

NumBytes 2

nameditem
	prompt	"Remote Boot Enable"
	  Choice "Boot Enable"
	    pos[0]=XXXXXX1Xb
	  Choice "Boot Disable"
	    pos[0]=XXXXXX0Xb
	Help
	 "Choice Remote Boot Enable/Disable"
nameditem
	Prompt	"Adapter Memory Location"
	  Choice "Segment D000"
	    pos[1]=01XXXXXXb
	    mem 0d0000h-0d7fffh
	  Choice "Segment C800"
	    pos[1]=10XXXXXXb
	    mem 0c8000h-0cffffh
	  Choice "Segment D800"
	    pos[1]=00XXXXXXb
	    mem 0d8000h-0dffffh
	  Choice "Segment C000"
	    pos[1]=11XXXXXXb
	    mem 0c0000h-0c7fffh
	Help
	"To configure this adapter you must choose the memory location the
	 adapter will use for it's BOOT ROM.  There are four memory locations
	 that can be selected.	Under normal circumstances, select <Segment
	 D000>."

nameditem
	prompt "IRQ Channel"
	  Choice "IRQ3"
	    pos[1]=XX000XXXb
	    int 3
	  Choice "IRQ4"
	    pos[1]=XX001XXXb
	    int 4
	  Choice "IRQ5"
	    pos[1]=XX010XXXb
	    int 5
	  Choice "IRQ6"
	    pos[1]=XX011XXXb
	    int 6
	  Choice "IRQ7"
	    pos[1]=XX100XXXb
	    int 7
	  Choice "IRQ9"
	    pos[1]=XX101XXXb
	    int 9
	  Choice "IRQ10"
	    pos[1]=XX110XXXb
	    int 10
	  Choice "IRQ11"
	    pos[1]=XX111XXXb
	    int 11
	  Help
	  "This is the interrupt request channel select. Under normal circumst-
	   ances, select channel 3"

nameditem
	prompt "IO Port Selection"
	  Choice "IO base 300" pos[1]=XXXXX011b io 0300h-031fh
	  Choice "IO base 200" pos[1]=XXXXX111b io 0200h-021fh
	  Choice "IO base 220" pos[1]=XXXXX110b io 0220h-023fh
	  Choice "IO base 240" pos[1]=XXXXX101b io 0240h-025fh
	  Choice "IO base 260" pos[1]=XXXXX100b io 0260h-027fh
	  Choice "IO base 320" pos[1]=XXXXX010b io 0320h-033fh
	  Choice "IO base 340" pos[1]=XXXXX001b io 0340h-035fh
	  Choice "IO base 360" pos[1]=XXXXX000b io 0360h-037fh
	  Help
	  "IO port select. Under normal circustance, select port 0300h-031fh."
