; Stepping Stone MUX 50/60/80 Adapter
; Copyright (c) Cumulus Corporation 1987. All rights reserved

AdapterId 7023h

AdapterName "Stepping Stone MUX 50/60/80 Adapter"

Numbytes 1

NamedItem
	Prompt "Port Address Auto Selected at "

	choice " 210h "
	pos[1]=00001000b
	io 210h - 210h

	choice " 220h "
	pos[1]=00010000b
	io 220h - 220h

	choice " 230h "
	pos[1]=00011000b
	io 230h - 230h

	choice " 240h "
	pos[1]=00100000b
	io 240h - 240h

	choice " 250h "
	pos[1]=00101000b
	io 250h - 250h

	choice " 260h "
	pos[1]=00110000b
	io 260h - 260h

	choice " 270h "
	pos[1]=00111000b
	io 270h - 270h

	choice " 280h "
	pos[1]=01000000b
	io 280h - 280h

	choice " 290h "
	pos[1]=01001000b
	io 290h - 290h

	choice " 2A0h "
	pos[1]=01010000b
	io 2a0h - 2a0h

	choice " 2B0h "
	pos[1]=01011000b
	io 2b0h - 2b0h

	choice " 2C0h "
	pos[1]=01100000b
	io 2c0h - 2c0h

	choice " 2D0h "
	pos[1]=01101000b
	io 2d0h - 2d0h

	choice " 2E0h "
	pos[1]=01110000b
	io 2e0h - 2e0h

	choice " 2F0h "
	pos[1]=01111000b
	io 2f0h - 2f0h

	choice " 300h "
	pos[1]=10000000b
	io 300h - 300h

	Help

	"This is the IO port address the software uses to control the
	 external floppy drive. The address is automatically selected 
	 by the system therefore manual configuration is not required."
