
AdapterID 00FC7h

AdapterName  "Wizard Attached Processor"

NumBytes 4

FixedResources
      pos[1]=xxx0xxxxb
      pos[3]=00000000b

InitProg 30

nameditem
        Prompt  "Adapter I/O Location"
          Choice "Base Address 8AA0"
            pos[0]=XXXX000Xb
            io 8AA0h-8AAFh

        Help
        "Base Address must be 8AA0"

nameditem
        Prompt  "DMA Arbitration Level"
          Choice  "Level D"
            pos[1]=XXXX1101b
            arb 0Dh
          Choice  "Level E"
            pos[1]=XXXX1110b
            arb 0Eh
          Choice  "Level 8"
            pos[1]=XXXX1000b
            arb 8
          Choice  "Level 9"
            pos[1]=XXXX1001b
            arb 9
          Choice  "Level A"
            pos[1]=XXXX1010b
            arb 0Ah
          Choice  "Level B"
            pos[1]=XXXX1011b
            arb 0Bh
          Choice  "Level C"
            pos[1]=XXXX1100b
            arb 0Ch
        Help
        "This selects the DMA Arbitration level the adapter will use to
         transfer data. Under normal circumstances, select <Level D>."



nameditem
        Prompt  "Interrupt Level"
          Choice  "Level 11"
            pos[2]=XXXXXX01b
            int 0bh
          Choice  "Level 10"
            pos[2]=XXXXXX00b
            int 0ah
          Choice  "Level 15"
            pos[2]=XXXXXX10b
            int 0fh
          Choice  "Level 5"
            pos[2]=XXXXXX11b
            int 5

        Help
        "Interrupt Level. This controls the Interrupt line the adapter
         will use to signal the host. Under normal circumstances,
         select <Level 11>."
