AdapterId 0F5Fh


AdapterName "GSS MC1000"


NumBytes 3

NamedItem

Prompt	"Enable/Disable Adapter"

Choice	" Adapter Enabled "    pos[0]=XXXXXXX1b
Choice	" Adapter Disabled "   pos[0]=XXXXXXX0b

Help

"This controls whether the adapter is enabled or not.
Use the Enabled setting for normal use.
Use the Disabled setting if you are not using
the adapter and enabling it causes a conflict
with another device."

NamedItem

Prompt "Hardware Registers"

choice "  BC0 to BCF " pos[1]=XX010XXXb  io 0BC0h-0BCFh
choice "  7C0 to 7CF " pos[1]=XX001XXXb  io 07C0h-07CFh
choice "  FC0 to FCF " pos[1]=XX011XXXb  io 0FC0h-0FCFh
choice "  13C0 to 13CF " pos[1]=XX100XXXb  io 13C0h-13CFh
choice "  17C0 to 17CF " pos[1]=XX101XXXb  io 17C0h-17CFh
choice "  1BC0 to 1BCF " pos[1]=XX110XXXb  io 1BC0h-1BCFh
choice "  1FC0 to 1FCF " pos[1]=XX111XXXb  io 1FC0h-1FCFh

Help

"Determines the range of i/o addresses used.
These include the 34010 host port registers and the
command and status registers.  The addresses in
this range cannot be used by another installed device."

NamedItem

Prompt "Color Palette addresses"

choice "  3C6 to 3C9 " pos[1]=XXXXX000b
choice "  7C6 to 7C9 " pos[1]=XXXXX001b  io 07C6h-07C9h
choice "  BC6 to BC9 " pos[1]=XXXXX010b  io 0BC6h-0BC9h
choice "  FC6 to FC9 " pos[1]=XXXXX011b  io 0FC6h-0FC9h
choice "  13C6 to 13C9 " pos[1]=XXXXX100b  io 013C6h-013C9h
choice "  17C6 to 17C9 " pos[1]=XXXXX101b  io 017C6h-017C9h
choice "  1BC6 to 1BC9 " pos[1]=XXXXX110b  io 01BC6h-01BC9h
choice "  1FC6 to 1FC9 " pos[1]=XXXXX111b  io 01FC6h-01FC9h

Help

"Determines the range of i/o addresses used by the
color palette.	If mapped to 3C6-3C9, the  color palette
shadows the VGA color palette."


NamedItem

Prompt "Interrupt Level"

choice " Channel 9 "  pos[0]=1000XXXXb  INT 9
choice " Channel 10 "  pos[0]=0001XXXXb  INT 10
choice " Channel 11 "  pos[0]=0100XXXXb  INT 11
choice " Channel 12 "  pos[0]=0010XXXXb  INT 12

Help

"Determines the interrupt level used by ."


NamedItem

Prompt "Pixel Clock Frequency"
choice " 50 Mhz "  pos[0]=XXXXX01Xb
choice " 64 Mhz "  pos[0]=XXXXX00Xb
choice " 36 Mhz "  pos[0]=XXXXX10Xb
Help

"Determines the pixel clock frequency and therefore the display
resolution.  64 Mhz provides 1024 x 768 resolution, 38 Mhz
provides 800 x 600 resolution."


NamedItem

Prompt "Bus Arbitration Level"

choice "Level 7"      pos[3]=1X0X0111b ARB 7
choice "Level 3"      pos[3]=1X0X0011b ARB 3
choice "Level 1"      pos[3]=1X0X0001b ARB 1
choice "Level 5"      pos[3]=1X0X0101b ARB 5

Help

"Determines the bus arbitration level for the 34010 bus master."

NamedItem

Prompt "Horizontal Sync Polarity"
choice " Negative "  pos[0]=XXXX0XXXb
choice " Positive "  pos[0]=XXXX1XXXb
Help

"Sets the horizontal composite sync polarity for high
resolution graphics modes."


