
AdapterId 07F7Eh

AdapterName  "ORCHID RamQuest EXTRA"

NumBytes 4

fixedResources
;       ** This is the "unused" bit in register 102
        pos[0]=XXXXXX0Xb
;       ** This is the 102 shadow mask (0=>writable)
        pos[2]=XXXX0XXXb
;       ** 
        pos[3]=XXXXXXX0b

NamedItem
       Prompt  "Adapter BIOS Location"
           Choice "Segment C000"
               pos[0]=01000XXXb  mem 0c0000h-0c0fffh
           Choice "Segment C100"
               pos[0]=01001XXXb  mem 0c1000h-0c1fffh
           Choice "Segment C200"
               pos[0]=01010XXXb  mem 0c2000h-0c2fffh
           Choice "Segment C300"
               pos[0]=01011XXXb  mem 0c3000h-0c3fffh
           Choice "Segment C400"
               pos[0]=01100XXXb  mem 0c4000h-0c4fffh
           Choice "Segment C500"
               pos[0]=01101XXXb  mem 0c5000h-0c5fffh
           Choice "Segment C600"
               pos[0]=01110XXXb  mem 0c6000h-0c6fffh
           Choice "Segment C700"
               pos[0]=01111XXXb  mem 0c7000h-0c7fffh
           Choice "DISABLED"
               pos[0]=00000XXXb

   Help
       "To configure this adapter you must choose the memory location
       the adapter will use for it's BIOS ROM.  If multiple Ramquest
       Extra adapters are installed, ONLY ONE needs to be assigned a
       BIOS location - the others can be DISABLED.  There are eight
       memory locations that can be selected.  Under normal
       circumstances, select <Segment C000>."

NamedItem
        Prompt "Connector 1"
           choice "SERIAL_1"  pos[3]=XXXX001Xb  io 03f8h-03ffh  int 4
           choice "SERIAL_2"  pos[3]=XXXX010Xb  io 02f8h-02ffh  int 3
           choice "SERIAL_3"  pos[3]=XXXX011Xb  io 3220h-3227h  int 3
           choice "SERIAL_4"  pos[3]=XXXX100Xb  io 3228h-322fh  int 3
           choice "SERIAL_5"  pos[3]=XXXX101Xb  io 4220h-4227h  int 3
           choice "SERIAL_6"  pos[3]=XXXX110Xb  io 4228h-422fh  int 3
           choice "SERIAL_7"  pos[3]=XXXX111Xb  io 5220h-5227h  int 3
           choice "DISABLED"  pos[3]=XXXX000Xb

   Help
"No Help Yet..."

NamedItem
        Prompt "Connector 2"
           choice "SERIAL_1"  pos[3]=X001XXXXb  io 03f8h-03ffh  int 4
           choice "SERIAL_2"  pos[3]=X010XXXXb  io 02f8h-02ffh  int 3
           choice "SERIAL_3"  pos[3]=X011XXXXb  io 3220h-3227h  int 3
           choice "SERIAL_4"  pos[3]=X100XXXXb  io 3228h-322fh  int 3
           choice "SERIAL_5"  pos[3]=X101XXXXb  io 4220h-4227h  int 3
           choice "SERIAL_6"  pos[3]=X110XXXXb  io 4228h-422fh  int 3
           choice "SERIAL_8"  pos[3]=X111XXXXb  io 5228h-522fh  int 3
           choice "DISABLED"  pos[3]=X000XXXXb
   Help
"No Help Yet..."

NamedItem
       Prompt "Start Address    (DO NOT CHANGE!)"
           choice "(not set)"    pos[1]=00000000b
           choice "1408K"        pos[1]=00010110b
           choice "1920K"        pos[1]=00011110b
           choice "2432K"        pos[1]=00100110b
           choice "2944K"        pos[1]=00101110b
           choice "3456K"        pos[1]=00110110b
           choice "3968K"        pos[1]=00111110b
           choice "4480K"        pos[1]=01000110b
           choice "4992K"        pos[1]=01001110b
           choice "5504K"        pos[1]=01010110b
           choice "6016K"        pos[1]=01011110b
           choice "6526K"        pos[1]=01100110b
           choice "7040K"        pos[1]=01101110b
           choice "7552K"        pos[1]=01110110b
           choice "8064K"        pos[1]=01111110b
           choice "8576K"        pos[1]=10000110b
           choice "9088K"        pos[1]=10001110b
           choice "9600K"        pos[1]=10010110b
           choice "10112K"       pos[1]=10011110b
           choice "10624K"       pos[1]=10100110b
           choice "11136K"       pos[1]=10101110b
           choice "11648K"       pos[1]=10110110b
           choice "12160K"       pos[1]=10111110b
           choice "12672K"       pos[1]=11000110b
           choice "13184K"       pos[1]=11001110b
           choice "13696K"       pos[1]=11010110b
           choice "14208K"       pos[1]=11011110b
           choice "14720K"       pos[1]=11100110b

   Help
"No Help Yet..."

NamedItem
       Prompt "Installed Memory (DO NOT CHANGE!)"
           choice "   0K" pos[0]=XXXXXX0XB
                          pos[2]=XXXXX111B
           choice " 512K" pos[0]=XXXXXX0XB
                          pos[2]=XXXXX000B

           choice "1024K" pos[0]=XXXXXX1XB
                          pos[2]=XXXXX000B

           choice "1536K" pos[0]=XXXXXX0XB
                          pos[2]=XXXXX001B

           choice "2048K" pos[0]=XXXXXX1XB
                          pos[2]=XXXXX001B

           choice "2560K" pos[0]=XXXXXX0XB
                          pos[2]=XXXXX010B

           choice "3072K" pos[0]=XXXXXX1XB
                          pos[2]=XXXXX010B

           choice "3584K" pos[0]=XXXXXX0XB
                          pos[2]=XXXXX011B

           choice "4096K" pos[0]=XXXXXX1XB
                          pos[2]=XXXXX011B

           choice "4608K" pos[0]=XXXXXX0XB
                          pos[2]=XXXXX100B

           choice "5120K" pos[0]=XXXXXX1XB
                          pos[2]=XXXXX100B

           choice "6144K" pos[0]=XXXXXX1XB
                          pos[2]=XXXXX101B

           choice "6656K" pos[0]=XXXXXX0XB
                          pos[2]=XXXXX110B

           choice "8192K" pos[0]=XXXXXX1XB
                          pos[2]=XXXXX111B

   Help
"No Help Yet..."

;NamedItem
;        Prompt "BOARD I/O"
;           choice "DISABLED"  pos[2]=0001XXXXb
;           choice "Option 1"  pos[2]=0011XXXXb  io 0200h-0207h
;           choice "Option 2"  pos[2]=0101XXXXb  io 0300h-0307h
;           choice "Option 3"  pos[2]=0111XXXXb  io 1200h-1207h
;           choice "Option 4"  pos[2]=1001XXXXb  io 1300h-1307h
;           choice "Option 5"  pos[2]=1011XXXXb  io 2200h-2207h
;           choice "Option 6"  pos[2]=1101XXXXb  io 2300h-2307h
;           choice "Option 7"  pos[2]=1111XXXXb  io 3200h-3207h
;
;   Help
;"No Help Yet..."

