;
; Version: 1.00
;
; (C) Copyright IBM Corp. 1991
; All rights reserved.
;

AdapterId 0EFE8h

AdapterName  "FaxConcentrator Adapter/A"

NumBytes 2

NamedItem

        Prompt "Facsimile Port"

        choice "FACSIMILE_1"

                pos[0] = 0000XXXXb
                pos[1] = 01000010b
                io 4140h - 4143h
                int 4
                mem 0D0000h - 0D1FFFh

        choice "FACSIMILE_2"

                pos[0] = 0001XXXXb
                pos[1] = 01001010b
                io 4144h - 4147h
                int 4
                mem 0D2000h - 0D3FFFh

        choice "FACSIMILE_3"

                pos[0] = 0010XXXXb
                pos[1] = 01010010b
                io 4148h - 414Bh
                int 4
                mem 0D4000h - 0D5FFFh

        choice "FACSIMILE_4"

                pos[0] = 0011XXXXb
                pos[1] = 01011010b
                io 414Ch - 414Fh
                int 4
                mem 0D6000h - 0D7FFFh

        choice "FACSIMILE_5"

                pos[0] = 0100XXXXb
                pos[1] = 01100010b
                io 4150h - 4153h
                int 4
                mem 0D8000h - 0D9FFFh

        choice "FACSIMILE_6"

                pos[0] = 0101XXXXb
                pos[1] = 01101010b
                io 4154h - 4157h
                int 4
                mem 0DA000h - 0DBFFFh

        choice "FACSIMILE_7"

                pos[0] = 0110XXXXb
                pos[1] = 01110010b
                io 4158h - 415Bh
                int 4
                mem 0DC000h - 0DDFFFh

        choice "FACSIMILE_8"

                pos[0] = 0111XXXXb
                pos[1] = 01111010b
                io 415Ch - 415Fh
                int 4
                mem 0DE000h - 0DFFFFh


  Help

"This port can be assigned as a facsimile port (FACSIMILE_1
through FACSIMILE_8).  Use the F5=Previous and the F6=Next
keys to change this assignment in the 'Change configuration'
window.  Conflicting assignments are marked with an asterisk
and must be changed to use the adapter."

