
AdapterId	07520h
AdapterName     "ALR Micro Channel AT Imbedded Adapter"
NumBytes        4

FixedResources	pos[1]= XXXXXXXXb pos[2] = XXXXXXXXb pos[3] = 00000011b arb 3
   
NamedItem
Prompt  "Adapter ROM Location"
Choice   " Segment D000"   pos[1]=XX100XXXb    mem 0D0000h-0D3FFFh
Choice   " Segment C800"   pos[1]=XX010XXXb    mem 0C8000h-0CBFFFh
Choice   " Segment CC00"   pos[1]=XX011XXXb    mem 0CC000h-0CFFFFh
Choice   " Segment D400"   pos[1]=XX101XXXb    mem 0D4000h-0D7FFFh
Choice   " Segment D800"   pos[1]=XX110XXXb    mem 0D8000h-0DBFFFh
Choice   " Segment DC00"   pos[1]=XX111XXXb    mem 0DC000h-0DFFFFh
Help
"To configure this adapter you must choose the memory location
the adapter will use for its BIOS ROM. There are seven memory 
locations that can be selected.  Under normal circumstances, 
select <Segment C800>."

NamedItem
Prompt   "Adapter I/O Address"
Choice   "I/O Address 01F0h-01FFh"    pos[1]=00XXXXXXb    io 01F0h-01FFh
Choice   "I/O Address 11F0h-11FFh"    pos[1]=01XXXXXXb    io 11F0h-11FFh
Choice   "I/O Address 21F0h-21FFh"    pos[1]=10XXXXXXb    io 21F0h-21FFh
Choice   "I/O Address 31F0h-31FFh"    pos[1]=11XXXXXXb    io 31F0h-31FFh
Help
"You must choose the I/O location for the adapter to interface to
the imbedded drive. There are four possible I/O spaces. Under normal
circumstances, select <I/O Address 01F0h-01FFh>."

NamedItem
Prompt 	"Interrupt Level"
Choice 	"INT 14"		      pos[0]=0XXXXXXXb	  int 14
Choice 	"INT 15"		      pos[0]=1XXXXXXXb	  int 15
Help
"You must choose the interrupt level for the adapter to interrupt 
the system. Default condition is <INT 14>."

