; IBM PS/2 Adapter/A for Ethernet Networks
; Adapter Description File
;
AdapterId      0EFD4h
AdapterName     "IBM PS/2 Adapter/A for Ethernet Networks"
NumBytes        4

NamedItem
    Prompt   "Adapter I/O Range"
         Choice "00800 - 0081F"
             pos[0]=0000XXXXb
             io 00800h-0081Fh
         Choice "01800 - 0181F"
             pos[0]=0001XXXXb
             io 01800h-0181Fh
         Choice "02800 - 0281F"
             pos[0]=0010XXXXb
             io 02800h-0281Fh
         Choice "03800 - 0381F"
             pos[0]=0011XXXXb
             io 03800h-0381Fh
         Choice "04800 - 0481F"
             pos[0]=0100XXXXb
             io 04800h-0481Fh
         Choice "05800 - 0581F"
             pos[0]=0101XXXXb
             io 05800h-0581Fh
Help
"Select the Adapter I/O Range where the adapter will reside.  There
are 6 locations that may be selected.  Press F5(Previous) or F6(Next)
to change the assignment.  Conflicting assignments are marked with an
asterisk (*) and must be changed."
   
NamedItem
    Prompt  "RAM Address Range"
         Choice "8K: C0000 - C1FFF"
             pos[1]=0x000000b
             mem 00C0000h-00C1FFFh
         Choice "8K: C2000 - C3FFF"
             pos[1]=0x000001b
             mem 00C2000h-00C3FFFh
         Choice "8K: C4000 - C5FFF"
             pos[1]=0x000010b
             mem 00C4000h-00C5FFFh
         Choice "8K: C6000 - C7FFF"
             pos[1]=0x000011b
             mem 00C6000h-00C7FFFh
         Choice "8K: C8000 - C9FFF"
             pos[1]=0x000100b
             mem 00C8000h-00C9FFFh
         Choice "8K: CA000 - CBFFF"
             pos[1]=0x000101b
             mem 00CA000h-00CBFFFh
         Choice "8K: CC000 - CDFFF"
             pos[1]=0x000110b
             mem 00CC000h-00CDFFFh
         Choice "8K: CE000 - CFFFF"
             pos[1]=0x000111b
             mem 00CE000h-00CFFFFh
         Choice "8K: D0000 - D1FFF"
             pos[1]=0x001000b
             mem 00D0000h-00D1FFFh
         Choice "8K: D2000 - D3FFF"
             pos[1]=0x001001b
             mem 00D2000h-00D3FFFh
         Choice "8K: D4000 - D5FFF"
             pos[1]=0x001010b
             mem 00D4000h-00D5FFFh
         Choice "8K: D6000 - D7FFF"
             pos[1]=0x001011b
             mem 00D6000h-00D7FFFh
         Choice "8K: D8000 - D9FFF"
             pos[1]=0x001100b
             mem 00D8000h-00D9FFFh
         Choice "8K: DA000 - DBFFF"
             pos[1]=0x001101b
             mem 00DA000h-00DBFFFh
         Choice "8K: DC000 - DDFFF"
             pos[1]=0x001110b
             mem 00DC000h-00DDFFFh
         Choice "8K: DE000 - DFFFF"
             pos[1]=0x001111b
             mem 00DE000h-00DFFFFh
;
         Choice "16K: C0000 - C3FFF"
             pos[1]=0x010000b
             mem 00C0000h-00C3FFFh
         Choice "16K: C2000 - C5FFF"
             pos[1]=0x010001b
             mem 00C2000h-00C5FFFh
         Choice "16K: C4000 - C7FFF"
             pos[1]=0x010010b
             mem 00C4000h-00C7FFFh
         Choice "16K: C6000 - C9FFF"
             pos[1]=0x010011b
             mem 00C6000h-00C9FFFh
         Choice "16K: C8000 - CBFFF"
             pos[1]=0x010100b
             mem 00C8000h-00CBFFFh
         Choice "16K: CA000 - CDFFF"
             pos[1]=0x010101b
             mem 00CA000h-00CDFFFh
         Choice "16K: CC000 - CFFFF"
             pos[1]=0x010110b
             mem 00CC000h-00CFFFFh
         Choice "16K: CE000h -D1FFF"
             pos[1]=0x010111b
             mem 00CE000h-00D1FFFh
         Choice "16K: D0000 - D3FFF"
             pos[1]=0x011000b
             mem 00D0000h-00D3FFFh
         Choice "16K: D2000 - D5FFF"
             pos[1]=0x011001b
             mem 00D2000h-00D5FFFh
         Choice "16K: D4000 - D7FFF"
             pos[1]=0x011010b
             mem 00D4000h-00D7FFFh
         Choice "16K: D6000 - D9FFF"
             pos[1]=0x011011b
             mem 00D6000h-00D9FFFh
         Choice "16K: D8000 - DBFFF"
             pos[1]=0x011100b
             mem 00D8000h-00DBFFFh
         Choice "16K: DA000 - DDFFF"
             pos[1]=0x011101b
             mem 00DA000h-00DDFFFh
         Choice "16K: DC000 - DFFFF"
             pos[1]=0x011110b
             mem 00DC000h-00DFFFFh
Help
"Choose the adapter RAM system address.  There are 31 memory locations
that may be selected.  The 16K choices provide the adapter with more
system to adapter buffer space.  Press F5(Previous) or F6(Next) to
change the assignment.  Conflicting assignments, marked with an
asterisk (*), must be changed."

NamedItem
    Prompt "ROM BIOS Address Range"
         Choice "8K: C8000 - C9FFF"
             pos[2]=XX000100b
             mem 00C8000h-00C9FFFh
         Choice "8K: CA000 - CBFFF"
             pos[2]=XX000101b
             mem 00CA000h-00CBFFFh
         Choice "8K: CC000 - CDFFF"
             pos[2]=XX000110b
             mem 00CC000h-00CDFFFh
         Choice "8K: CE000 - CFFFF"
             pos[2]=XX000111b
             mem 00CE000h-00CFFFFh
         Choice "8K: D0000 - D1FFF"
             pos[2]=XX001000b
             mem 00D0000h-00D1FFFh
         Choice "8K: D2000 - D3FFF"
             pos[2]=XX001001b
             mem 00D2000h-00D3FFFh
         Choice "8K: D4000 - D5FFF"
             pos[2]=XX001010b
             mem 00D4000h-00D5FFFh
         Choice "8K: D6000 - D7FFF"
             pos[2]=XX001011b
             mem 00D6000h-00D7FFFh
         Choice "8K: D8000 - D9FFF"
             pos[2]=XX001100b
             mem 00D8000h-00D9FFFh
         Choice "8K: DA000 - DBFFF"
             pos[2]=XX001101b
             mem 00DA000h-00DBFFFh
         Choice "8K: DC000 - DDFFF"
             pos[2]=XX001110b
             mem 00DC000h-00DDFFFh
         Choice "8K: DE000 - DFFFF"
             pos[2]=XX001111b
             mem 00DE000h-00DFFFFh
;        Choice "   Disabled  "
;            pos[2]=XX110000b
Help
"Choose the memory address the adapter will use for its ROM BIOS.
There are 12 memory locations that may be selected.  Press
F5(Previous) or F6(Next) to change the assignment.  Conflicting
assignments, marked with an asterisk (*), must be changed."

NamedItem
    Prompt  "Interrupt Level"
         Choice "Level 3"
             pos[3]=XXXX0001b
             int 3
         Choice "Level 4"
             pos[3]=XXXX0101b
             int 4
         Choice "Level 10"
             pos[3]=XXXX1001b
             int 10
         Choice "Level 14"
             pos[3]=XXXX1101b
             int 14
Help
"Some LAN operating systems may require that a unique interrupt level
be selected.  To avoid conflicts, there are four choices available."

NamedItem
Prompt  "Remote Program Load"
         Choice "Enabled"
             pos[3]=XXX0XXXXb
         Choice "Disabled"
             pos[3]=XXX1XXXXb
Help
"The Remote Program Load (RPL) option allows the system to execute
BIOS code on the adapter.  RPL only needs to be disabled if there is
more than one RPL adpater in the system."
