AdapterId 06FE4h

AdapterName "DigiBoard PS-COM/16"

NumBytes 4

NamedItem

Prompt "UART Address Range"

choice "0x3000 -> 0x307F" pos[3]=xxxxxxx0b
	      pos[2]=01100000b
	      io 03000h-0307fh
choice "0x4000 -> 0x407F" pos[3]=xxxxxxx0b
	      pos[2]=10000000b
	      io 04000h-0407fh
choice "0x4100 -> 0x417F" pos[3]=xxxxxxx0b
	      pos[2]=10000010b
	      io 04100h-0417fh
choice "0x4200 -> 0x427F" pos[3]=xxxxxxx0b
	      pos[2]=10000100b
	      io 04200h-0427fh
choice "0x4300 -> 0x437F" pos[3]=xxxxxxx0b
	      pos[2]=10000110b
	      io 04300h-0437fh
choice "0x5000 -> 0x507F" pos[3]=xxxxxxx0b
	      pos[2]=10100000b
	      io 05000h-0507fh
choice "0x6000 -> 0x607F" pos[3]=xxxxxxx0b
	      pos[2]=11000000b
	      io 06000h-0607fh
choice "0x7000 -> 0x707F" pos[3]=xxxxxxx0b
	      pos[2]=11100000b
	      io 07000h-0707fh

Help

"No Help Available"


NamedItem

Prompt "Com2 Status"

choice "Disabled"
	      pos[3]=xx00xxxxb
choice "Enabled"
	      pos[3]=xx11xxxxb
	      io 02f8h-02ffh
Help

"No help is Available"


NamedItem

Prompt "Interrupt Status Register Start Address"

choice "0x3080 -> 0x3081" pos[1]=00110000b
	       pos[0]=1000000xb
	       io 03080h-03081h
choice "0x4080 -> 0x4081" pos[1]=01000000b
	       pos[0]=1000000xb
	       io 04080h-04081h
choice "0x4180 -> 0x4181" pos[1]=01000001b
	       pos[0]=1000000xb
	       io 04180h-04181h
choice "0x4280 -> 0x4281" pos[1]=01000010b
	       pos[0]=1000000xb
	       io 04280h-04281h
choice "0x4380 -> 0x4381" pos[1]=01000011b
	       pos[0]=1000000xb
	       io 04380h-04381h
choice "0x5080 -> 0x5081" pos[1]=01010000b
	       pos[0]=1000000xb
	       io 05080h-05081h
choice "0x6080 -> 0x6081" pos[1]=01100000b
	       pos[0]=1000000xb
	       io 06080h-06081h
Help

"No help is Available"

NamedItem

Prompt "Interrupt Select"

choice "INT 3" pos[3]=xxxx000xb   int 3
choice "INT 4" pos[3]=xxxx001xb   int 4
choice "INT 5" pos[3]=xxxx010xb   int 5
choice "INT 7" pos[3]=xxxx011xb   int 7
choice "INT 10" pos[3]=xxxx100xb  int 10
choice "INT 11" pos[3]=xxxx101xb  int 11
choice "INT 12" pos[3]=xxxx110xb  int 12
choice "INT 15" pos[3]=xxxx111xb  int 15

Help

"No Help is currently available"
