;****************************************************************************
;*
;* @704F.ADF
;* MPCA/MC Adapter Description File
;*
;****************************************************************************
;*
;* The content of this document is NCR intellectual property of the NCR
;* corporation.  It is to be treated as strictly confidential and not to be
;* disclosed, reproduced, or used except as authorized in writing by NCR in
;* connection with the manufacture, maintenance and use of the NCR equipment
;* to which it pertains.
;*
;* Copyright (c) 1990 NCR Corporation Workstation Products Division
;*
;****************************************************************************
;*
;* version      : 1.00.00
;* author       : Karl Reinke
;* start date   : 5/7/90
;* stop date    : 5/7/90
;*
;* revision history:
;*   DATE   | NUMBER  | AUTHOR |               ?                    
;* ---------+---------+--------+------------------------------------
;*  7/10/90 | 1.00.00 | KR     | Release version
;*          |         |        |
;*
;****************************************************************************
AdapterId 0704Fh

AdapterName "NCR MPCA/MC Adapter"

NumBytes 2


NamedItem	

Prompt  "Adapter enable/disable function"

	Choice "Adapter Enabled"
		POS[0]=0XXXXXX1b
	Choice "Adapter Disabled"
		POS[0]=0XXXXXX0b

Help

"You can enable or disable the NCR MPCA/MC adapter by using this
option.

Use the F5=Previous and the F6=Next keys to enable or disable the
adapter."


NamedItem	

Prompt	"Adapter I/O Base Address"

	Choice "Base address: 000380"
		POS[0]=0XXX000Xb	IO	000380h - 00038Fh
	Choice "Base address: 000400"
		POS[0]=0XXX001Xb	IO	000400h - 00040Fh
	Choice "Base address: 000480"
		POS[0]=0XXX010Xb	IO	000480h - 00048Fh
	Choice "Base address: 000500"
		POS[0]=0XXX011Xb	IO	000500h - 00050Fh
	Choice "Base address: 000580"
		POS[0]=0XXX100Xb	IO	000580h - 00058Fh
	Choice "Base address: 000600"
		POS[0]=0XXX101Xb	IO	000600h - 00060Fh
	Choice "Base address: 000680"
		POS[0]=0XXX110Xb	IO	000680h - 00068Fh
	Choice "Base address: 000700"
		POS[0]=0XXX111Xb	IO	000700h - 00070Fh

Help

"You can configure the NCR MPCA/MC adapter for 8 different I/O
base address ranges.  If there is more than one MPCA/MC adapter
in the PC, set each adapter to a different base address.  An
asterisk indicates a conflicting I/O address.

Use the F5=Previous and the F6=Next keys to change the base
address setting."


NamedItem	

Prompt	"Adapter Interrupt Request Level"

	Choice "IRQ Level 10"	
        	POS[0]=0000XXXXb	INT 10
	Choice "IRQ Level 11"
		POS[0]=0001XXXXb	INT 11
	Choice "IRQ Level 12"
		POS[0]=0010XXXXb	INT 12
	Choice "IRQ Level 14"
		POS[0]=0011XXXXb	INT 14
	Choice "IRQ Level 3"	
        	POS[0]=0100XXXXb	INT 3
	Choice "IRQ Level 4"
		POS[0]=0101XXXXb	INT 4
	Choice "IRQ Level 5"
		POS[0]=0110XXXXb	INT 5
	Choice "IRQ Level 7"
		POS[0]=0111XXXXb	INT 7

Help

"The NCR MPCA/MC adapter can use one of eight different interrupt
request levels.  The MPCA/MC can share an IRQ level with any other
adapter, but to avoid a decrease in system performance select
an unique IRQ level for the adapter.  An asterisk indicates a
shared IRQ level.

Use the F5=Previous and the F6=Next keys to change the interrupt
request level assignment."


NamedItem

Prompt "Adapter Board ID Number"

	Choice "Board ID = 1"
		POS[1]=00000000b
	Choice "Board ID = 2"
		POS[1]=00000001b
	Choice "Board ID = 3"
		POS[1]=00000010b
	Choice "Board ID = 4"
		POS[1]=00000011b

Help

"This item assigns an unique board ID number to the NCR MPCA/MC
adapter.  This allows the operation of up to four MPCA/MC adapters
in one PC if each adapter is given a different board ID number.

Use the F5 = Previous and the F6 = Next keys to select the board
ID number."

;
; end of @704F.ADF
;
