
AdapterID 062B6h

AdapterName  "Arco Electronics AC-1079 SLIM Drive Adapter"

NumBytes 2

fixedresources
	pos[0]=0X0XXXXXb

nameditem
	Prompt	"Adapter Memory Location"

	  Choice "Segment DC00" pos[0]=XXXX110Xb mem 0dc000h-0dffffh
	  Choice "Segment D800" pos[0]=XXXX101Xb mem 0d8000h-0dbfffh
	  Choice "Segment D400" pos[0]=XXXX100Xb mem 0d4000h-0d7fffh
	  Choice "Segment D000" pos[0]=XXXX011Xb mem 0d0000h-0d3fffh
	  Choice "Segment CC00" pos[0]=XXXX010Xb mem 0cc000h-0cffffh
	  Choice "Segment C800" pos[0]=XXXX001Xb mem 0c8000h-0cbfffh
	  Choice "ROM DISABLE"  pos[0]=XXXX000Xb 
	Help
	"Select the ROM segment for the ARCO IDE adapter."

nameditem
	Prompt	"IO Address"
	  Choice    "2510-251F" pos[0]=XXX0XXXXb io 2510h-251fh
	  Choice    "2520-252F" pos[0]=XXX1XXXXb io 2520h-252fh
	Help
	"The Adapter may be located in one of the following I/O address
	 locations: 2510-251F or 2520-252F"
nameditem
    Prompt  "Redundant Write For Mirroring"
      Choice   "No " pos[0]=X0XXXXXXb
      Choice   "Yes" pos[0]=X1XXXXXXb
    Help
    "You can use this option to mirror your drive"

