


AdapterID 0FFF8h

AdapterName  "S36/38 Work Station Emulation Adapter"

NumBytes 3

NamedItem Prompt "interrupt level"

choice "interrupt 5" pos[2]=00000101b int 5
choice "interrupt 3" pos[2]=00000011b int 3
choice "interrupt 4" pos[2]=00000100b int 4
choice "interrupt 7" pos[2]=00000111b int 7

   Help
"Choose the hardware interrupt level for the 5250 Work Station Emulation Adapter."

NamedItem prompt "memory address"
choice "DC000 - DFFFF"
   POS[0] = 1101110xb
   POS[1] = 00001111b
   MEM 0DC000h - 0DFFFFh
choice "D8000 - DBFFF"
   POS[0] = 1101100xb
   POS[1] = 00001111b
   MEM 0D8000h - 0DBFFFh
choice "D4000 - D7FFF"
   POS[0] = 1101010xb
   POS[1] = 00001111b
   MEM 0D4000h - 0D7FFFh
choice "D0000 - D3FFF"
   POS[0] = 1101000xb
   POS[1] = 00001111b
   MEM 0D0000h - 0D3FFFh
choice "CC000 - CFFFF"
   POS[0] = 1100110xb
   POS[1] = 00001111b
   MEM 0CC000h - 0CFFFFh
choice "C8000 - CBFFF"
   POS[0] = 1100100xb
   POS[1] = 00001111b
   MEM 0C8000h - 0CBFFFh
choice "C4000 - C7FFF"
   POS[0] = 1100010xb
   POS[1] = 00001111b
   MEM 0C4000h - 0C7FFFh
choice "C0000 - C3FFF"
   POS[0] = 1100000xb
   POS[1] = 00001111b
   MEM 0C0000h - 0C3FFFh

   Help
"Choose the memory address range for the 5250 adapter."
