AdapterId 06dd4h

AdapterName "FasTalk 2/V.32/5, 2/V.32/42b"

NumBytes 1

NamedItem
	Prompt "Asynchronous Modem Port" 
      choice "Serial_1"  pos[0]=10x01xxxb io 03f8h-03ffh  int 4 
      choice "Serial_2"  pos[0]=10x00xxxb io 02f8h-02ffh  int 3 
      choice "Serial_3"  pos[0]=10x10xxxb io 3220h-3227h  int 3 
      choice "Serial_4"  pos[0]=10x11xxxb io 3228h-322fh  int 3 
      choice "DISABLED"  pos[0]=00x00xxxb 
 
Help 
"The Asynchronous portion of this modem 
can be assigned to use Serial_1 through Serial_
4 or DISABLED.  Use the F5=Previous and the 
F6=Next keys to change the assigment. 
Conflicting assignments are marked with an 
asterisk and must be changed." 
 
