;
; Version:      1.00
;
; (C) Copyright International Business Machines Corporation 1988
; All rights reserved.
;

AdapterID 0EDD7h

AdapterName  "RAS Adapter"

NumBytes 4

FixedResources
        pos[0]=0000000Xb
        pos[2]=XXXXXXXXb
        pos[3]=XXXXXXXXb
        io 1AE0h-1AEFh

NamedItem
        Prompt  "Interrupt Level"
          Choice  "Interrupt 11"        pos[1]=XXXXXX00b int 11
          Choice  "Interrupt 10"        pos[1]=XXXXXX01b int 10
          Choice  "Interrupt  9"        pos[1]=XXXXXX10b int  9
        Help
        "Choose the hardware interrupt level for the RAS Adapter.
         The preferred interrupt level is 11, but the adapter can
         operate on any of the three levels if necessary.
         Use the F5=Previous and the F6=Next keys to change this
         assignment. Conflicting assignments are marked with
         an asterisk and must be changed."
