AdapterId  5103h
AdapterName "Creative Labs, Inc. - SOUND BLASTER PRO MCV CT5330 "
NumBytes 4

NamedItem
Prompt "Base I/O Address"

choice "220 Hex"  pos[0]=00100101b
                  pos[1]=11110000b
                             io 0220h-022Fh 0230h-0237h 0200h-0207h 0380h-038Fh

choice "240 Hex"  pos[0]=01000101b
                  pos[1]=11110000b
                             io 0240h-024Fh 0250h-0257h 0200h-0207h 0380h-038Fh

Help
"The Base Address can be assigned to 220H or 240H.
 Use [F5] for previous and [F6] for next."

NamedItem
Prompt "DMA channel"

choice "DMA 1" pos[2]=11110001b arb 1 
choice "DMA 0" pos[2]=11110000b arb 0 
choice "DMA 3" pos[2]=11110011b arb 3

Help
"The DMA channel can be assigned at channel 0, 1 and 3.
 Use [F5] for previous and [F6] for next."

NamedItem
Prompt "Interrupt"

choice "IRQ7 selected " pos[3]=11001010b int 7
choice "IRQ5 selected " pos[3]=11011010b int 5
choice "IRQ3 selected " pos[3]=11101010b int 3

Help
"The interrupt can be assigned at interrupt 3,5 or 7.
 Use [F5] for previous and [F6] for next."

