;***************************************************************************
;* Copyright (C) 1989 by NCR Corporation    This program		   *
;* contains proprietary and confidential information.  All rights reserved *
;* except as may be permitted by prior written consent.                    *
;*************************************************************************** 

AdapterId 004Fh

AdapterName "NCR 53C710 SCSI Host Adapter Board"

NumBytes 4


NamedItem
  Prompt "Host Adapter Board Interrupt Level"
      choice "INT LEVEL 5"     pos[0]=X100XXXXb   INT 5
      choice "INT LEVEL 9"     pos[0]=X101XXXXb   INT 9
      choice "INT LEVEL 14"     pos[0]=X110XXXXb   INT 14
        
  Help
"Set the Host Adapter Board Interrupt Level so it will not conflict with 
other interrupting devices.  Diskettes are usually level 6."



NamedItem
      Prompt "I/O Address Select"
      choice "300"        pos[0]=XXXX010Xb   io 00300h-00345h
      choice "200"        pos[0]=XXXX001Xb   io 00200h-00245h
      choice "400"        pos[0]=XXXX011Xb   io 00400h-00445h
      choice "500"        pos[0]=XXXX100Xb   io 00500h-00545h
      choice "600"        pos[0]=XXXX101Xb   io 00600h-00645h
      choice "Disabled"	  pos[0]=XXXX000Xb

Help
"You may set the NCR SCSI adapter to any one of the I/O
Addresses listed.  The first choice is recommended.  If 
your selection conflicts with an I/O address already 
assigned in your system, it will be marked with an asterisk
and you must select an alternate address."


NamedItem
   Prompt "Static Ram Starting Address"
        choice "D0000h-D1FFFh"  pos[1]=11000XXXb  mem 0D0000h-0D1FFFh
	choice "C0000h-C1fffh"	pos[1]=10000XXXb  mem 0C0000h-0C1fffh
	choice "C2000h-C3FFFh"	pos[1]=10001XXXb  mem 0C2000h-0C3FFFh
	choice "C4000h-C5FFFh"	pos[1]=10010XXXb  mem 0C4000h-0C5FFFh
	choice "C6000h-C7FFFh"	pos[1]=10011XXXb  mem 0C6000h-0C7FFFh
	choice "C8000h-C9FFFh"	pos[1]=10100XXXb  mem 0C8000h-0C9FFFh
	choice "CA000h-CBFFFh"	pos[1]=10101XXXb  mem 0CA000h-0CBFFFh
	choice "CC000h-CDFFFh"	pos[1]=10110XXXb  mem 0CC000h-0CDFFFh
	choice "CE000h-CFFFFh"	pos[1]=10111XXXb  mem 0CE000h-0CFFFFh
	choice "D2000h-D3FFFh"	pos[1]=11001XXXb  mem 0D2000h-0D3FFFh
	choice "D4000h-D5FFFh"	pos[1]=11010XXXb  mem 0D4000h-0D5FFFh
	choice "D6000h-D7FFFh"	pos[1]=11011XXXb  mem 0D6000h-0D7FFFh
	choice "D8000h-D9FFFh"	pos[1]=11100XXXb  mem 0D8000h-0D9FFFh
	choice "DA000h-DBFFFh"	pos[1]=11101XXXb  mem 0DA000h-0DBFFFh
	choice "DC000h-DDFFFh"	pos[1]=11110XXXb  mem 0DC000h-0DDFFFh
	choice "DE000h-DFFFFh"	pos[1]=11111XXXb  mem 0DE000h-0DFFFFh
	choice "Disabled"       pos[1]=00000XXXb
   Help
"Set the Static Ram Starting Address to avoid conflict with other
adapters which use the extended ROM area for ROM or RAM.  The 
default is C8000h."


NamedItem
   Prompt "Host Adapter Board Logical ID"
	choice "7"		pos[1]=XXXXX111b
	choice "6"		pos[1]=XXXXX110b
	choice "5"		pos[1]=XXXXX101b
	choice "4"		pos[1]=XXXXX100b
	choice "3"		pos[1]=XXXXX011b
	choice "2"		pos[1]=XXXXX010b
	choice "1"		pos[1]=XXXXX001b
	choice "0"		pos[1]=XXXXX000b

Help
   "Set the Host Adapter Board Logical ID to avoid conflict when
   performing adapter to adapter I/O.  The default is 7."
