; IBM PS/2 Adapter/A for Ethernet(TM) Networks
; Adapter Description File
; Version 1.00
;
AdapterId       0EFE5h
AdapterName     "IBM PS/2 Adapter/A for Ethernet(TM) Networks"
NumBytes        4
FixedResources  pos[1]=XXXXXXX0b pos[3]=000X01XXb

NamedItem
    Prompt   "Adapter I/O Range"
         Choice   "0200 - 021F"
             pos[0]=0010000Xb
             io 0200h-021Fh
         Choice   "0220 - 023F"
             pos[0]=0010001Xb
             io 0220h-023Fh
         Choice   "0280 - 029F"
             pos[0]=0010100Xb
             io 0280h-029Fh
         Choice   "0240 - 025F"
             pos[0]=0010010Xb
             io 0240h-025Fh
         Choice   "0260 - 027F"
             pos[0]=0010011Xb
             io 0260h-027Fh
         Choice   "02A0 - 02BF"
             pos[0]=0010101Xb
             io 02A0h-02BFh
         Choice   "02C0 - 02DF"
             pos[0]=0010110Xb
             io 02C0h-02DFh
         Choice   "0300 - 031F"
             pos[0]=0011000Xb
             io 0300h-031Fh
         Choice   "0320 - 033F"
             pos[0]=0011001Xb
             io 0320h-033Fh
         Choice   "0340 - 035F"
             pos[0]=0011010Xb
             io 0340h-035Fh
         Choice   "0360 - 037F"
             pos[0]=0011011Xb
             io 0360h-037Fh
         Choice   "0380 - 039F"
             pos[0]=0011100Xb
             io 0380h-039Fh
Help
"To configure this adapter, select the I/O address range where the
adapter will reside.  There are 12 locations that may be
selected.  Press F5(Previous) or F6(Next) to change the assignment.
Conflicting assignments are marked with an asterisk (*) and must be
changed.  Under normal circumstances, select <0200 - 021F>."

NamedItem
    Prompt  "RAM Address Range (16K Bytes)"
         Choice   "C8000 - CBFFF"
             pos[1]=1100101Xb
             mem 0C8000h-0CBFFFh
         Choice   "CC000 - CFFFF"
             pos[1]=1100111Xb
             mem 0CC000h-0CFFFFh
         Choice   "D8000 - DBFFF"
             pos[1]=1101101Xb
             mem 0D8000h-0DBFFFh
         Choice   "DC000 - DFFFF"
             pos[1]=1101111Xb
             mem 0DC000h-0DFFFFh
         Choice   "D0000 - D3FFF"
             pos[1]=1101001Xb
             mem 0D0000h-0D3FFFh
         Choice   "D4000 - D7FFF"
             pos[1]=1101011Xb
             mem 0D4000h-0D7FFFh
         Choice   "C0000 - C3FFF"
             pos[1]=1100001Xb
             mem 0C0000h-0C3FFFh
         Choice   "C4000 - C7FFF"
             pos[1]=1100011Xb
             mem 0C4000h-0C7FFFh
Help
"To configure this adapter, choose the memory location the adapter's
16K bytes of RAM will use.  There are 8 memory locations that may be
selected.  Press F5(Previous) or F6(Next) to change the assignment.
Conflicting assignments, marked with an asterisk (*), must be changed.
Under normal circumstances, select <C8000 - CBFFF>."

NamedItem
    Prompt  "ROM BIOS Address Range (16K Bytes)"
         Choice   "D4000 - D7FFF"
             pos[2]=11010100b
             mem 0D4000h-0D7FFFh
         Choice   "C8000 - CBFFF"
             pos[2]=11001000b
             mem 0C8000h-0CBFFFh
         Choice   "CC000 - CFFFF"
             pos[2]=11001100b
             mem 0CC000h-0CFFFFh
         Choice   "D8000 - DBFFF"
             pos[2]=11011000b
             mem 0D8000h-0DBFFFh
         Choice   "DC000 - DFFFF"
             pos[2]=11011100b
             mem 0DC000h-0DFFFFh
         Choice   "D0000 - D3FFF"
             pos[2]=11010000b
             mem 0D0000h-0D3FFFh
;        Choice   "Disabled"
;            pos[2]=XXXXXX10b
Help

"To configure this adapter, choose the memory location the adapter
will use for its ROM BIOS.  There are 6 memory locations that may be
selected.  Press F5(Previous) or F6(Next) to change the assignment.
Conflicting assignments, marked with an asterisk (*), must be changed.
Under normal circumstances, select <D4000 - D7FFF>."

NamedItem
    Prompt  "Interrupt Level"
         Choice   "Level 3"
             pos[3]=XXXXXX00b
             int  3
         Choice   "Level 4"
             pos[3]=XXXXXX01b
             int  4
         Choice   "Level 10"
             pos[3]=XXXXXX10b
             int  10
         Choice   "Level 15"
             pos[3]=XXXXXX11b
             int  15
Help
"This selects the adapter interrupt level.  Under normal
circumstances, select <Level 3>."

NamedItem
    Prompt  "Remote Program Load"
         Choice   "Enabled"
             pos[3]=XXX0XXXXb
         Choice   "Disabled"
             pos[3]=XXX1XXXXb
Help
"Enabling the Remote Program Load (RPL) option allows the system to
execute BIOS code on the adapter.  Only one adapter in the
system should have RPL enabled."
