; CuRAM 32 Plus Extended Memory Multifunction Adapter
; Copyright (c) Cumulus Corporation 1989, 1990. All rights reserved
; Adapter Definition File Version 1.0

AdapterId 7025h

AdapterName "CuRAM 32 Plus Extended Memory Multifunction Adapter"

Numbytes 4

;FixedResources
;	pos[1]=x111xxxxb



NamedItem

	Prompt "ROM Address"

	choice "C8000 - C8FFFF"
		pos[3]=11101000b
		mem 0C8000h-0C8FFFh

	choice "C9000 - C9FFFF"
		pos[3]=11101001b
		mem 0C9000h-0C9FFFh

	choice "CA000 - CAFFFF"
		pos[3]=11101010b
		mem 0CA000h-0CAFFFh

	choice "CB000 - CBFFFF"
		pos[3]=11101011b
		mem 0CB000h-0CBFFFh

	choice "CC000 - CCFFFF"
		pos[3]=11101100b
		mem 0CC000h-0CCFFFh

	choice "CD000 - CDFFFF"
		pos[3]=11101101b
		mem 0CD000h-0CDFFFh

	choice "CE000 - CEFFFF"
		pos[3]=11101110b
		mem 0CE000h-0CEFFFh

	choice "CF000 - CFFFFF"
		pos[3]=11101111b
		mem 0CF000h-0CFFFFh

	choice "D0000 - D0FFFF"
		pos[3]=11110000b
		mem 0D0000h-0D0FFFh

	choice "D1000 - D1FFFF"
		pos[3]=11110001b
		mem 0D1000h-0D1FFFh

	choice "D2000 - D2FFFF"
		pos[3]=11110010b
		mem 0D2000h-0D2FFFh

	choice "D3000 - D3FFFF"
		pos[3]=11110011b
		mem 0D3000h-0D3FFFh

	choice "D4000 - D4FFFF"
		pos[3]=11110100b
		mem 0D4000h-0D4FFFh

	choice "D5000 - D5FFFF"
		pos[3]=11110101b
		mem 0D5000h-0D5FFFh

	choice "D6000 - D6FFFF"
		pos[3]=11110110b
		mem 0D6000h-0D6FFFh

	choice "D7000 - D7FFFF"
		pos[3]=11110111b
		mem 0D7000h-0D7FFFh

	choice "D8000 - D8FFFF"
		pos[3]=11111000b
		mem 0D8000h-0D8FFFh

	choice "D9000 - D9FFFF"
		pos[3]=11111001b
		mem 0D9000h-0D9FFFh

	choice "DA000 - DAFFFF"
		pos[3]=11111010b
		mem 0DA000h-0DAFFFh

	choice "DB000 - DBFFFF"
		pos[3]=11111011b
		mem 0DB000h-0DBFFFh

	choice "DC000 - DCFFFF"
		pos[3]=11111100b
		mem 0DC000h-0DCFFFh

	choice "DD000 - DDFFFF"
		pos[3]=11111101b
		mem 0DD000h-0DDFFFh

	choice "DE000 - DEFFFF"
		pos[3]=11111110b
		mem 0DE000h-0DEFFFh

	choice "DF000 - DFFFFF"
		pos[3]=11111111b
		mem 0DF000h-0DFFFFh

	choice "Disable ROM"
		pos[3]=11000000b



Help
	"Select ROM address range. Select [Disable ROM] option only when
	 no memory is installed on the Adapter."


NamedItem

	Prompt "Matched Memory Cycle"

	choice "Enable"
		pos[1]=0111xxxxb

	choice "Disable"
		pos[1]=1111xxxxb

Help
	"Enable Matched Memory Cycle if running on PS/2 Model 80 systems.
	Disable Matched Memory Cycle otherwise."


NamedItem

	Prompt "Serial Port"

	choice 	"Disable Serial Port"
		pos[0]=xxxxx0xxb

	choice "COM2 configuration"
		pos[0]=xxxx11xxb
		io 2f8h - 2ffh
		int 3	
	choice "COM1 configuration"
		pos[0]=xxxx01xxb
		io 3f8h - 3ffh
		int 4

	Help
	"If an optional Serial Communications Port is installed select 
	the desired COM port setting. Otherwise, please select the
	[Disable Serial Port] option"

NamedItem

	Prompt "Parallel Port Enable"

	choice "Disable parallel port"
		pos[0]=xxx0xxxxb

	choice "LPT2"
		pos[0]=1011xxxxb
		io 378h - 37bh
		int 7

	choice "LPT2 extended"
		pos[0]=0011xxxxb
		io 378h - 37bh
		int 7

	choice "LPT3"
		pos[0]=1101xxxxb
		io 278h - 27bh
		int 7

	choice "LPT3 extended"
		pos[0]=0101xxxxb
		io 278h - 27bh
		int 7

	choice "LPT1"
		pos[0]=1001xxxxb
		io 3BCh - 3BFh
		int 7

	choice "LPT1 extended"
		pos[0]=0001xxxxb
		io 3BCh - 3BFh
		int 7


	Help
	"If an optional Parallel Communications Port is installed select 
	the desired LPT port setting. Otherwise, please select the
	[Disable Parallel Port] option"
