
AdapterId 0EFEFh

AdapterName  "PC Network Adapter "

NumBytes 1

NamedItem

        Prompt "Type, Memory Location, Interrupt Level"

        choice "Primary, Mem 1, Int 2"

                pos[0] = 1X00010Xb
                io 0620h - 0627h
                int 2
                mem 0C8000h - 0CFFFFh

        choice "Primary, Mem 2, Int 2"

                pos[0] = 1X00001Xb
                io 0620h - 0627h
                int 2
                mem 0D0000h - 0D7FFFh

        choice "Primary, Mem 3, Int 2"

                pos[0] = 1X00011Xb
                io 0620h - 0627h
                int 2
                mem 0D8000h - 0DFFFFh

        choice "Primary, Mem 1, Int 3"

                pos[0] = 1X01010Xb
                io 0620h - 0627h
                int 3
                mem 0C8000h - 0CFFFFh

        choice "Primary, Mem 2, Int 3"

                pos[0] = 1X01001Xb
                io 0620h - 0627h
                int 3
                mem 0D0000h - 0D7FFFh

        choice "Primary, Mem 3, Int 3"

                pos[0] = 1X01011Xb
                io 0620h - 0627h
                int 3
                mem 0D8000h - 0DFFFFh

        choice "Alternate, Mem 1, Int 3"

                pos[0] = 0X01110Xb
                io 0628h - 062Fh
                int 3
                mem 0CE000h - 0CFFFFh

        choice "Alternate, Mem 2, Int 3"

                pos[0] = 0X01101Xb
                io 0628h - 062Fh
                int 3
                mem 0D6000h - 0D7FFFh

        choice "Alternate, Mem 3, Int 3"

                pos[0] = 0X01111Xb
                io 0628h - 062Fh
                int 3
                mem 0DE000h - 0DFFFFh

        choice "RPL, Mem 1, Int 2"

                pos[0] = 1X10010Xb
                io 0620h - 0627h
                int 2
                mem 0C8000h - 0CFFFFh

        choice "RPL, Mem 2, Int 2"

                pos[0] = 1X10001Xb
                io 0620h - 0627h
                int 2
                mem 0D0000h - 0D7FFFh

        choice "RPL, Mem 3, Int 2"

                pos[0] = 1X10011Xb
                io 0620h - 0627h
                int 2
                mem 0D8000h - 0DFFFFh

        choice "RPL, Mem 1, Int 3"

                pos[0] = 1X11010Xb
                io 0620h - 0627h
                int 3
                mem 0C8000h - 0CFFFFh

        choice "RPL, Mem 2, Int 3"

                pos[0] = 1X11001Xb
                io 0620h - 0627h
                int 3
                mem 0D0000h - 0D7FFFh

        choice "RPL, Mem 3, Int 3"

                pos[0] = 1X11011Xb
                io 0620h - 0627h
                int 3
                mem 0D8000h - 0DFFFFh

  Help

"To configure this adapter you may choose the adapter type,
memory location, and interrupt level. The three adapter types
are primary, alternate, and Remote Program Load (RPL). There are
three memory locations for each adapter type. The primary adapter
and the RPL adapter may use one of two interrupt levels, while
the alternate adapter uses interrupt level 3.  Use the
F5=Previous and the F6=Next keys to change this assignment. Conflicting
assignments are marked with an asterisk and must be
changed."

