;***************************************************************************
;* Copyright (C) 1990 by NCR Corporation    This program		   *
;* contains proprietary and confidential information.  All rights reserved *
;* except as may be permitted by prior written consent.                    *
;*************************************************************************** 

AdapterId 00000h

AdapterName "NCR PARALLEL BUS MEMORY CARD "

NumBytes 10

NamedItem

	Prompt "EDAC error check I/O address"
	Choice "0xDE00"		io 0de00h-0de07h	pos[4]=00000XXXb 
	Choice "0xDE08"		io 0de08h-0de0fh	pos[4]=00001XXXb 
	Choice "0xDE10"		io 0de10h-0de17h	pos[4]=00010XXXb 
	Choice "0xDE18"		io 0de18h-0de1fh	pos[4]=00011XXXb 
	Choice "DEFAULT"	pos[4]=00000XXXb
	Help
"This is the starting address of the eight-byte error check register block
for this memory card. "

FixedResources
	pos[5]=11011110b
; pos 5 sets the high byte of the EDAC error check register to 0xDE
	pos[9]=X0100000b
; pos 9 bit 5 sets single board post to enable




