; @621c.ADF  Ver 1.02
;
; file @67E1.ADF used to configure the
; Extended TTY 16 Port Controller Card


AdapterId       0621ch

AdapterName     "NCR  16 Port Serial Controller/MC"

NumBytes        4


FixedResources
pos[0]=0xxxxxxxb
;bit 7 = 0: download mode
pos[1]=xxxxx00xb
;bit 2 = 0, bit 1 = 0: block select 0
pos[3]=110xxxxxb
;bit 7 = 1: enable chck; bit 6 = 1: no status; bit 5 = 0: async ready


NamedItem
Prompt  "Dual Port Address"
choice "0D0000H" pos[0]=x110100xb MEM 0d0000h-0d3fffh
choice "0D4000H" pos[0]=x110101xb MEM 0d4000h-0d7fffh
choice "0D8000H" pos[0]=x110110xb MEM 0d8000h-0dbfffh
choice "0DC000H" pos[0]=x110111xb MEM 0dc000h-0dffffh
choice "0C0000H" pos[0]=x110000xb MEM 0c0000h-0c3fffh
choice "0C4000H" pos[0]=x110001xb MEM 0c4000h-0c7fffh
choice "0C8000H" pos[0]=x110010xb MEM 0c8000h-0cbfffh
choice "0CC000H" pos[0]=x110011xb MEM 0cc000h-0cffffh
Help
"This selects the address of this controller's dual port RAM.
 Under normal circumstances, select <0D0000H>.
 Use the F5=Previous and the F6=Next keys to change this
 assignment.  Conflicting assignments are marked with an
 asterisk and must be changed to use the adapter."


NamedItem
Prompt "Interrupt Level"
choice "IRQ 3 " pos[3]=xxxx0000b  INT 3
choice "IRQ 4 " pos[3]=xxxx0001b  INT 4
choice "IRQ 5 " pos[3]=xxxx0010b  INT 5
choice "IRQ 7 " pos[3]=xxxx0011b  INT 7
choice "IRQ 9 " pos[3]=xxxx0100b  INT 9
choice "IRQ 10" pos[3]=xxxx0101b  INT 10
choice "IRQ 11" pos[3]=xxxx0110b  INT 11
choice "IRQ 12" pos[3]=xxxx0111b  INT 12
choice "No IRQ" pos[3]=xxxx1000b
Help
"This selects the Interrupt Level this controller will use.
Interrupts can also be disabled.  Under normal cicumstances, 
select <IRQ 3>.  Use the F5=Previous and the F6=Next keys to 
change this assignment."

;end of file

