AdapterId 07083h

AdapterName "AST Advantage/2 -386 Adapter"

NumBytes 4

NamedItem
      Prompt "Memory size configuration"
      choice "MEMORY DISABLED"  POS[0]=X000XXXXb
      choice "1 MEGA BYTES"     POS[0]=X001XXXXb
      choice "2 MEGA BYTES"     POS[0]=X010XXXXb
      choice "4 MEGA BYTES"     POS[0]=X011XXXXb
      choice "5 MEGA BYTES"     POS[0]=X100XXXXb
      choice "8 MEGA BYTES"     POS[0]=X101XXXXb


Help
" Memory Size Configuration indicates the amount of memory in
Bank0 and Bank1.  For one megabyte (MB), Bank0 is populated only.
Two MB's consists of Bank0 and Bank1 having one MB each.  Four MB's
consists of 4 MB's in Bank0 and none in Bank1.  Five MB's will have
one MB in Bank0 and four MB's in Bank1.  Eight MB's consists of four
MB's in Bank0 and four MB's in Bank1.   "

NamedItem
      Prompt "Wait State selection"
      choice "0 WAIT STATES"  pos[1]=1XXXXXXXb
      choice "1 WAIT STATE"   pos[1]=0XXXXXXXb

Help
" An additional wait state is inserted during any memory access when
  the choice '1 WAIT STATE' is made ."
