
AdapterID 000C4h

AdapterName  "Racore 16/4 Token-Ring Adapter"

NumBytes 3

FixedResources
	pos[0]=X1XXX1XXb

nameditem
        Prompt  "I/O Address"
          Choice  "I/O A20 - A2F"
            pos[1]=XXXXXX01b
            io 0A20h-0A2Fh
          Choice  "I/O A00 - A0F"
            pos[1]=XXXXXX00b
            io 0A00h-0A0Fh
          Choice  "I/O A40 - A4F"
            pos[1]=XXXXXX10b
            io 0A40h-0A4Fh
          Choice  "I/O A60 - A6F"
            pos[1]=XXXXXX11b
            io 0A60h-0A6Fh
        Help
        "This selects the I/O addresses the adapter will use. A20h is
	 recommended for most applications, especially for 3270 and
 	 AS400 connectivity."

nameditem
        Prompt  "Interrupt (IRQ)"
          Choice  "IRQ2 (IRQ9)"
            pos[1]=XXXX01XXb
            int 2
          Choice  "IRQ3"
            pos[1]=XXXX00XXb
            int 3
          Choice  "IRQ10"
            pos[1]=XXXX10XXb
            int 10
          Choice  "IRQ11"
            pos[1]=XXXX11XXb
            int 11
        Help
        "Interrupt (IRQ) select.  This selects which interrupt (IRQ) line to use.
	 IRQ2 is recommended for most applications, especially for 3270 and AS400
	 connectivity."

nameditem
        Prompt  "ROM Address"
          Choice "CC000 - CDFFF (8K)"
            pos[1]=XX00XXXXb
	    pos[2]=XXXX1XX0b
            mem 0CC000h-0CDFFFh
          Choice "D0000 - D1FFF (8K)"
            pos[1]=XX01XXXXb
	    pos[2]=XXXX1XX0b
            mem 0D0000h-0D1FFFh
          Choice "D8000 - D9FFF (8K)"
            pos[1]=XX10XXXXb
	    pos[2]=XXXX1XX0b
            mem 0D8000h-0D9FFFh
          Choice "DC000 - DDFFF (8K)"
            pos[1]=XX11XXXXb
	    pos[2]=XXXX1XX0b
            mem 0DC000h-0DDFFFh
	  Choice "ROM DISABLED"
	    pos[1]=XX00XXXXb
	    pos[2]=XXXX0XX0b
        Help
        "Select the memory location the adapter will use for the ROM. The ROM
	 must be enabled to allow system software to access the
	 Burned-In-Address (BIA). If the ROM is disabled, a network address
	 must be supplied by the user. This can be accomplished by specifying
	 a network address on the command line, or in a configuration file
	 when software is loaded. Refer to driver specific documentation for
	 details on specifying a network address. The ROM must be enabled if
	 Remote Program Load (RPL) is desired."

nameditem
        Prompt  "BUS Master Arbitration Level"
          Choice "Level 8"
            pos[1]=00XXXXXXb
            pos[0]=XX10XXXXb
            arb 8
          Choice "Level 9"
	    pos[1]=01XXXXXXb
            pos[0]=XX10XXXXb
            arb 9
          Choice "Level A"
            pos[1]=10XXXXXXb
            pos[0]=XX10XXXXb
            arb 0ah
          Choice "Level B"
	    pos[1]=11XXXXXXb
            pos[0]=XX10XXXXb
            arb 0bh
          Choice "Level C"
            pos[1]=00XXXXXXb
            pos[0]=XX11XXXXb
            arb 0ch
          Choice "Level D"
	    pos[1]=01XXXXXXb
            pos[0]=XX11XXXXb
            arb 0dh
          Choice "Level E"
            pos[1]=10XXXXXXb
            pos[0]=XX11XXXXb
            arb 0eh
          Choice "Level 0"
            pos[1]=00XXXXXXb
            pos[0]=XX00XXXXb
            arb 0
          Choice "Level 1"
	    pos[1]=01XXXXXXb
            pos[0]=XX00XXXXb
            arb 1
          Choice "Level 2"
	    pos[1]=10XXXXXXb
            pos[0]=XX00XXXXb
            arb 2
          Choice "Level 3"
	    pos[1]=11XXXXXXb
            pos[0]=XX00XXXXb
            arb 3
          Choice "Level 5"
	    pos[1]=01XXXXXXb
            pos[0]=XX01XXXXb
            arb 5
          Choice "Level 6"
            pos[1]=10XXXXXXb
            pos[0]=XX01XXXXb
            arb 6
          Choice "Level 7"
	    pos[1]=11XXXXXXb
            pos[0]=XX01XXXXb
            arb 7
	Help
	"Select the Arbitration Level in which the card competes to become
         Bus Master and transfer data to and from the Host.  The higher the
         number, the lower the priority.  Not all levels may be available to
         the user.  Conflicts are marked with an asterisk."

nameditem
	Prompt "BUS Master DMA Transfer Mode"
	  Choice "Maximum Burst"
	    pos[2]=XXXXXX1Xb
	  Choice "Minimum Burst"
	    pos[2]=XXXXXX0Xb
	Help
	"When transfering data, if Minimum Burst is selected, the adapter
	 will immediately release the bus if another adapter wishes to gain
	 control of the bus. If Maximum Burst is selected, the adapter will
	 continue transfering data up to 7.8 usec after detecting that
	 another adapter wishes to gain control of the bus. Maximum adapter
	 performance will be achieved by selecting Maximum Burst mode."

nameditem
	Prompt "BUS Master Streaming DMA Mode"
	  Choice "DISABLE"
	    pos[2]=XXXXX0XXb
	  Choice "ENABLE"
	    pos[2]=XXXXX1XXb
	Help
	"Enabling streaming DMA mode will allow the adapter to transfer data
	 using streaming DMA methods. Enabling this option will not have any
	 effect on machines which do not support streaming DMA."

nameditem
        Prompt  "BUS Arbitration Fairness"
          Choice "ENABLE"
            pos[0]=XXXXXX1Xb
          Choice "DISABLE"
            pos[0]=XXXXXX0Xb
        Help
        "If fairness is enabled during the bus arbitration process, the
	 adapter will not request the bus after a transfer has completed
	 until all other adapters which have requested the bus get a turn."

nameditem
        Prompt  "Ring Speed"
          Choice "16 Megabits/Sec"
            pos[0]=XXXX0XXXb
          Choice "4 Megabits/Sec"
            pos[0]=XXXX1XXXb
        Help
        "Select the data rate of the ring in which the adapter will run.
	 All adapters on the ring must run at the same speed. You can
	 choose between 4 and 16 megabits/second."

nameditem
        Prompt  "Connector/Cable Type"
          Choice "9 PIN (STP/Type 1)"
            pos[0]=0XXXXXXXb
          Choice "RJ45 (UTP/Type 3) or Fiber Optic"
            pos[0]=1XXXXXXXb
        Help
        "Specify which connector that the network cabling is attached to.
	 Normally, Shielded Twisted Pair (STP/Type 1 Cable) is connected to
	 the 9 PIN D connector, and Unshielded Twisted Pair (UTP/Type 3) is
	 connected to the RJ11/RJ45 connector. Be sure to select the 9 PIN
	 connector if you are using a UTP/Type 3 media filter attached to the
	 9 pin connector. Ensure that you have the proper Multi-station Access
	 Unit (MAU) for the cable type selected. Note that fiber optic or UTP
	 connectors are not available on all models."

