; Trantor T260 MicroChannel SCSI Host Adapter
; Adapter Descriptor File (ADF)
; Copyright (C) 1992, Trantor Systems, Ltd.
;
; Revised 10-01-92  RCB  First cut.
; Revised 11-05-92  RCB  Invert polarity of I/O & memory
;                        adrs select bits.


; We have an assigned id of 508eh.

adapterid 508eh
adaptername "Trantor T260 SCSI Host Adapter"


; We use four POS registers

numbytes 4


; The T260 SCSI interface is I/O mapped.
; One of the eight address options must be selected.

nameditem
prompt "I/O Port"
choice "360h - 36fh"  pos [1] = xxxxx000b  io 360h-36fh
choice "350h - 35fh"  pos [1] = xxxxx001b  io 350h-35fh
choice "340h - 34fh"  pos [1] = xxxxx010b  io 340h-34fh
choice "330h - 33fh"  pos [1] = xxxxx011b  io 330h-33fh
choice "260h - 26fh"  pos [1] = xxxxx100b  io 260h-26fh
choice "250h - 25fh"  pos [1] = xxxxx101b  io 250h-25fh
choice "240h - 24fh"  pos [1] = xxxxx110b  io 240h-24fh
choice "230h - 23fh"  pos [1] = xxxxx111b  io 230h-23fh
help
"The Trantor T260 SCSI Host Adapter uses 16 consecutive
port addresses. The port addresses used by the card must
not be used by any other cards in the computer. Use the 
F5 and F6 keys to select the desired port range."


; The 8k window (for the ROM) may occupy any of
; seven memory ranges.  The ROM may be disabled.

nameditem
prompt "ROM Address"
choice "ROM Disabled"     pos [1] = xx000xxxb
choice "c8000h - c9fffh"  pos [1] = xx001xxxb  mem 0c8000h-0c9fffh
choice "ca000h - cbfffh"  pos [1] = xx010xxxb  mem 0ca000h-0cbfffh
choice "ce000h - cffffh"  pos [1] = xx011xxxb  mem 0ce000h-0cffffh
choice "d0000h - d1fffh"  pos [1] = xx100xxxb  mem 0d0000h-0d1fffh
choice "d4000h - d5fffh"  pos [1] = xx101xxxb  mem 0d4000h-0d5fffh
choice "d8000h - d9fffh"  pos [1] = xx110xxxb  mem 0d8000h-0d9fffh
choice "dc000h - ddfffh"  pos [1] = xx111xxxb  mem 0dc000h-0ddfffh
help
"A Read Only Memory (ROM) is an option on the Trantor T260
SCSI Host Adapter. If you wish to use this option you must 
select the 8k range of memory which will be used by the ROM. 
You may also disable the ROM with this selection. Use the 
F5 and F6 keys to select the ROM address."


; The T260 provides 7 interrupt options.
; Interrupts may be disabled.

nameditem
prompt "Interrupt Channel"
choice "None"    pos [0] = xxxx000xb
choice "IRQ 3"   pos [0] = xxxx001xb  int 3
choice "IRQ 5"   pos [0] = xxxx010xb  int 5
choice "IRQ 7"   pos [0] = xxxx011xb  int 7
choice "IRQ 10"  pos [0] = xxxx100xb  int 10
choice "IRQ 12"  pos [0] = xxxx101xb  int 12
choice "IRQ 14"  pos [0] = xxxx110xb  int 14
choice "IRQ 15"  pos [0] = xxxx111xb  int 15
help
"The Trantor T260 SCSI Host Adapter supports interrupts.
Drivers such as ASPI (DOS), ADD (OS/2 2.0) and MiniPort
drivers (Windows NT) typically use interrupts.  Use the F5 
and F6 keys to select an interrupt channel."

