
AdapterID 06060h

AdapterName  "IDEAcomm 5251 7 LU short card"

NumBytes 2

fixedresources
        pos[0]=1XXXXXXXb

nameditem
        Prompt  "Adapter Memory Location"
          Choice "Segment C000"
            pos[1]=10110000b
            mem 0C0000h-0C7FFFh
          Choice "Segment C800"
            pos[1]=10110010b
            mem 0C8000h-0CFFFFh
          Choice "Segment D000"
            pos[1]=10110100b
            mem 0D0000h-0D7FFFh
          Choice "Segment D800"
            pos[1]=10110110b
            mem 0D8000h-0DFFFFh
          Choice  "RAM Disabled"
            pos[1]=00XXXXXXb
        Help
        "To configure this adapter you must choose the memory location the
         adapter will use for it's screen buffers.  There are eight memory
         locations that can be selected.  Under normal circumstances, select
         <Segment C000>."

NamedItem
        Prompt "Adapter IO location"

          Choice "IO Base 0368"
	    pos[0]=X0111111b
            io 0368h-0368h
          Choice "IO Base 0348"
	    pos[0]=X0111101b
            io 0348h-0348h
          Choice "IO Base 0328"
	    pos[0]=X0111011b
            io 0328h-0328h
          Choice "IO Base 0308"
	    pos[0]=X0111001b
            io 0308h-0308h

        Help
        "To configure this adapter you must choose the IO location the
         adapter will use for it's control register. There are four IO
         locations that can be selected.  Under normal circumstances, select
         <IO Base 0368>."


