
AdapterID 000C5h

AdapterName  "Racore 16/4 Token-Ring Adapter"

NumBytes 2

nameditem
        Prompt  "I/O Address"
          Choice  "I/O address A20h - A2Fh"
            pos[1]=XXXXXX01b
            io 0A20h-0A2Fh
          Choice  "I/O address A00h - A0Fh"
            pos[1]=XXXXXX00b
            io 0A00h-0A0Fh
          Choice  "I/O address A40h - A4Fh"
            pos[1]=XXXXXX10b
            io 0A40h-0A4Fh
          Choice  "I/O address A60h - A6Fh"
            pos[1]=XXXXXX11b
            io 0A60h-0A6Fh
        Help
        "This selects the I/O addresses the adapter will use."

nameditem
        Prompt  "Interrupt (IRQ)"
          Choice  "IRQ2 (IRQ9)"
            pos[1]=XXXX01XXb
            int 2
          Choice  "IRQ3"
            pos[1]=XXXX00XXb
            int 3
          Choice  "IRQ10"
            pos[1]=XXXX10XXb
            int 10
          Choice  "IRQ11"
            pos[1]=XXXX11XXb
            int 11
        Help
        "Interrupt (IRQ) select.  This selects which interrupt (IRQ) line to use."

nameditem
        Prompt  "Adapter ROM Location"
          Choice "Segment CC000 - CFFFF"
            pos[1]=XX00XXXXb
            mem 0CC000h-0CFFFFh
          Choice "Segment D0000 - D3FFF"
            pos[1]=XX01XXXXb
            mem 0D0000h-0D3FFFh
          Choice "Segment D8000 - DBFFF"
            pos[1]=XX10XXXXb
            mem 0D8000h-0DBFFFh
          Choice "Segment DC000 - DFFFF"
            pos[1]=XX11XXXXb
            mem 0DC000h-0DFFFFh
        Help
        "To configure this adapter you must choose the memory location the
         adapter will use for it's ROM.  There are four memory locations
         that can be selected."

nameditem
        Prompt  "BUS Master Arbitration Level"
          Choice "Level 6"
            pos[1]=10XXXXXXb
            pos[0]=XX01XXXXb
            arb 6
          Choice "Level 0"
            pos[1]=00XXXXXXb
            pos[0]=XX00XXXXb
            arb 0
          Choice "Level 1"
	    pos[1]=01XXXXXXb
            pos[0]=XX00XXXXb
            arb 1
          Choice "Level 2"
	    pos[1]=10XXXXXXb
            pos[0]=XX00XXXXb
            arb 2
          Choice "Level 3"
	    pos[1]=11XXXXXXb
            pos[0]=XX00XXXXb
            arb 3
          Choice "Level 5"
	    pos[1]=01XXXXXXb
            pos[0]=XX01XXXXb
            arb 5
          Choice "Level 7"
	    pos[1]=11XXXXXXb
            pos[0]=XX01XXXXb
            arb 7
          Choice "Level 8"
            pos[1]=00XXXXXXb
            pos[0]=XX10XXXXb
            arb 8
          Choice "Level 9"
	    pos[1]=01XXXXXXb
            pos[0]=XX10XXXXb
            arb 9
          Choice "Level A"
            pos[1]=10XXXXXXb
            pos[0]=XX10XXXXb
            arb 0ah
          Choice "Level B"
	    pos[1]=11XXXXXXb
            pos[0]=XX10XXXXb
            arb 0bh
          Choice "Level C"
            pos[1]=00XXXXXXb
            pos[0]=XX11XXXXb
            arb 0ch
          Choice "Level D"
	    pos[1]=01XXXXXXb
            pos[0]=XX11XXXXb
            arb 0dh
          Choice "Level E"
            pos[1]=10XXXXXXb
            pos[0]=XX11XXXXb
            arb 0eh
	Help
	"Select the Arbitration Level in which the card competes to become
         Bus Master and transfer data to and from the Host.  The higher the
         number, the lower the priority.  Not all levels may be available to
         the user.  Conflicts are marked with an asterisk."
nameditem
        Prompt  "Adapter Fairness Select"
          Choice "On"
            pos[0]=XXXXXX1Xb
          Choice "Off"
            pos[0]=XXXXXX0Xb
        Help
        "To configure this adapter you must choose if fairness is enabled in
         the bus arbitration process.  If fairness is enabled, after the adapter
         has transfered data and been pre-empted, it will not particapate for
         the bus again until everyone else who has requested the bus gets a turn."
nameditem
        Prompt  "Adapter Ring Speed Select"
          Choice "Speed = 16 Megabit"
            pos[0]=XXXX0XXXb
          Choice "Speed = 4 Megabit"
            pos[0]=XXXX1XXXb
        Help
        "To configure this adapter you must choose the speed of the ring in
         which the adapter will run.  All adapters on the ring must run at the
         same speed.  You can choose between 4 and 16 megabits/second."
nameditem
        Prompt  "Adapter RPL Enable Select"
          Choice "DISABLED"
            pos[0]=XXXXX0XXb
          Choice "ENABLED"
            pos[0]=XXXXX1XXb
        Help
        "To configure this adapter you must choose if the RPL (Remote Program Load
         EPROM is enabled or disabled.  The RPL program will load the operating
         system from a remote server allowing the host in which this adapter is
         installed to boot without a disk drive installed."
nameditem
        Prompt  "Adapter EPROM/RAM based MAC/LLC"
          Choice "ROM based MAC/LLC"
            pos[0]=X0XXXXXXb
          Choice "RAM based MAC/LLC (Down-load)"
            pos[0]=X1XXXXXXb
        Help
        "To configure this adapter you must choose if the adapter will boot from
         resident ROM or download its code from the host into its RAM and boot
         from that code.  If using the RPL feature, you need to select boot from
         ROM and be sure that you have the ROM's installed in the adapter board
         that will allow you to use these options."
nameditem
        Prompt  "Adapter Cable Type Selection"
          Choice "Type 1 cable (STP)"
            pos[0]=0XXXXXXXb
          Choice "Type 3 cable (UTP)"
            pos[0]=1XXXXXXXb
        Help
        "To configure this adapter you must choose if the adapter will use
         Shielded Twisted Pair (STP) type 1 cable or Unshielded Twisted Pair
         (UTP) type 3 cable.  The STP cable interface is provided on the
         9 pin D connector and the UTP cable interface is provided on the
         RJ11/RJ45 connector.  Ensure you have the proper Multi-station
         Access Unit (MAU) for the cable type selected."
