
AdapterId 0F7CEh

AdapterName  "Memory Expansion Option"

NumBytes 2

NamedItem
  Prompt "ROM Address Space"
    choice "Space 1"   pos[0]=XX1XX00Xb  pos[2]=0100XXXXb  mem 0C8000h-0C9FFFh
    choice "Space 2"   pos[0]=XX1XX00Xb  pos[2]=0101XXXXb  mem 0CA000h-0CBFFFh
    choice "Space 3"   pos[0]=XX1XX00Xb  pos[2]=0110XXXXb  mem 0CC000h-0CDFFFh
    choice "Space 4"   pos[0]=XX1XX00Xb  pos[2]=0111XXXXb  mem 0CE000h-0CFFFFh
    choice "Space 5"   pos[0]=XX1XX00Xb  pos[2]=1000XXXXb  mem 0D0000h-0D1FFFh
    choice "Space 6"   pos[0]=XX1XX00Xb  pos[2]=1001XXXXb  mem 0D2000h-0D3FFFh
    choice "Space 7"   pos[0]=XX1XX00Xb  pos[2]=1010XXXXb  mem 0D4000h-0D5FFFh
    choice "Space 8"   pos[0]=XX1XX00Xb  pos[2]=1011XXXXb  mem 0D6000h-0D7FFFh
    choice "Space 9"   pos[0]=XX1XX00Xb  pos[2]=1100XXXXb  mem 0D8000h-0D9FFFh
    choice "Space 10"  pos[0]=XX1XX00Xb  pos[2]=1101XXXXb  mem 0DA000h-0DBFFFh
    choice "Space 11"  pos[0]=XX1XX00Xb  pos[2]=1110XXXXb  mem 0DC000h-0DDFFFh
    choice "Space 12"  pos[0]=XX1XX00Xb  pos[2]=1111XXXXb  mem 0DE000h-0DFFFFh
    choice "Disabled"  pos[0]=XX0XX00Xb  pos[2]=0001XXXXb

  Help
   "The Expanded Memory Adapter ROM can be assigned to any one of 12 8k
    address spaces.  Use the F5=Previous and the F6=Next keys to change
    this assignment, if you are in the 'Change Configuration' window.  If
    the current assignment is marked with an asterisk, another adapter is
    using the address space.  Therefore the assignment must be changed to
    use this adapter."
