Source:
Procom Technology BBS:714-549-8614
Captured: 8-6-91 pse
~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~

PS/2 Products

Floppies                              SCSI
                                      
  30) External 5.25" Floppy           60) MC Enabler, SCSI Host Adapter
  31) External 3.5" Floppy            62) Internal SCSI Hard Drives
  32) External 40mb Tape Backup       63) External SCSI Hard Drive Sub-systems
                                      64) Removable Media Hard Disk Drive
                                      65) Erasable Optical Drive
				      66) CD ROM Drive
 				      67) 60-150mb Tape Backup Units
                                      68)1.3GB DAT Drive
                 
  Hard Disks  36) PhD Hard Disks for Model 25, 30, 30-286, and 50
	      37) Hidecard Drives for Model 25, 30, and 30-286
	      38) PIRA "Zero Slot" Hard Disk for Model 30-286
	      39) PIRA Hard Disk's for Model 50's
	      40) 65mb Hard Disk for Model 60 and 80
	      41) 155mb & 380mb Hard Disk for Model 60 and 80


PXF1200 & PXF360

Procom Technology's PS5.25 Series has been specifically designed for
PS/2 users whose computers support 3.5 inch floppy formats but have
large amounts of data stored on 5.25 inch formatted diskettes.  By
supporting both floppy formats on one computer, the user is able to
share files with others, regardless of floppy format.

FEATURES
-Does not occupy a slot or require an interface board.
-Works on all PS/2 systems.
-Drives may be installed as either drive A or B.
-Low power consumption; no power cord required.
-PXF1200 supports both high(1.2MB) and low (360KB) densities.
-DOS 3.30 and up, OS/2 and SCO Xenix 386 compatible.
-Supports IBM PTS/2 Personal Typing Systems.




ÿ


PXF1440/II

Procom Technology's PS3.5 Series provides floppy drive expansion
capability for PS/2 System users.  This slotless drive can read 720KB
and 1.44MB diskettes allowing PS/2 Model 25 & 30 users to upgrade
their 720KB floppy based machines to the higher denisity diskettes.


FEATURES

-Ideal for upgrading PS/2 Models 25 and 30 with high density 1.44MB
 diskette drives.
-Provides option for extra 3.5 inch diskette drive on all PS/2 systems.
-Does not require and expansion slot or interface card.
-Slim and compact design.
-Easy to install and operate.
-DOS and OS/2 compatible.
-Supports IBM PTS/2 Personal Typing Systems.


ÿ


PT40

Procom Technology's PT40 tape subsystem is a solid solution for
backing up, achieving and transporting valuable data between
locations.  The drives come complete with menu-driven backup
software, making them extremely cost effective.  And because they
plug directly into the floppy port on your PS/2 system, there is no
need for an expansion slot.  Al this makes the PT 40 the ideal choice
for all your critical backup needs.


FEATURES

-Includes powerful, easy-to-use, menu driven SYTOS backup software.
-Easily transportable.
-Optional expansion kits are available to facilitate backup and
 restore processes on multiple systems.
-Does not require an expansion slot or interface board.
-Supports PTS/2 Personal Typing Systems.

ÿ

PhD Series
20, 30, and 45mb Drives

Meeting mid-range storage capacity requirements, Procom Technology's
PH.D Series offers a superior line of cost-effective, highly reliable
3.5 inch Winchester disk drives with fast access times.  Developed
specifically for IBM's PS/2 25, 30, and 30-286 environment where
performance, reliability and efficiency are critical, PhD Series
drives have a very low power consumption and are configured
completely for quick installation into your IBM PS/2 system.


FEATURES

-Fast access times.
-High reliability and durability.
-Drives come complete with necessary mounting rails, face plates and
 controllers.
-Rugged design for maximum shock and vibration resistance.
-Ph.D 5045 replaces system drive without requiring an expansion slot.
-Can coexist with external floppy drives.


Hidecard Series

Procom Technology's HIDECARD Series is a superior line of reliable,
high performance card mounted hard disk drives that maximize data
storage capabilities while reducing data access times.  Designed to
meet the specific data storage needs for users of IBM PC, XT, AT and
compatible systems as well as PS/2 Models 30 and 20-286, the drives
mount into the systems without occupying a designated drive space.
Capacities include 20, 30 and 45MB.


FEATURE

-Allows users to retain both 3.5" diskette drives in their PS/2 Model
 30 and 30-286 systems.
-Fast access times as low as 25ms.
-Simple plug and play installation.

Notes:
-Only 20 and 45mb versions are compatible with IBM Model 30-286
-No Hidecards can coexist with another hard disk controller.
ÿ


PIRA 40, 100, & 200

The PIRA Series of hard disk subsystems provides owners of PS/2 Model
30 286 with the best of many worlds.  These zero-slot devices give
you AT Interrupt 13 software compatibility, up to five times the
available storage capacity in your system and performance increases
of up to 400%! All this at an unbeatable value.

FEATURES
-Does not require an expansion slot.
-Exceptional data transfe rates--up to 10Mbits/sec.
-1:1 interleave capacity.
-Supports Advanced NetWare 2.1x, DOS 3.30 and up, and OS/2 1.1.
-32K on board cache for full track buffering.
-Auto park and head lock.
 



ÿ


PIRA 50-100 & 200

The PIRA Series fo hard disk subsystems provides owners of PS/2
Models 50 and 50z with the best of many worlds.  These zero-slot
devices give you AT Interrupt 13 sofware compatibility, up to five
times the available storage capacity in your system and performance
increases of up to 400%!  All this at an unbeatable value.

FEATURES
-Does not require an expansion slot.
-Exceptional data transfer rates--up to 100Mbits/sec.
-1:1 interleave capacity.
-Supports Advanced NetWare 2.1x, DOS 3.30 and 4.0.
-32K on board cache for full track buffering.
-Auto park and head lock.




ÿ


HIPERII/65

Procom Technology's HIPER/II Series of high performance, high
capacity hard disk drives is the perfect solution for high capacity
PS/2 storage needs.  Designed specifically for IBM PS/2 Models 60 and
80, the 65MB version, an ST506 drive, provides a higher capacity
drive for users with -041 models and ST506 controllers.

FEATURES
-High speed data transfer rates and access times.
-Netware, DOS, OS/2 and Xenix compatible.
-Uses systme's existing hard disk controller.
-Plug and play installation.




ÿ


HIPER/II 155 & 380

Procom Technology's HIPER/II Series of high performance, high
capacity hard disk drives is the perfect solution for high capacity
PS/2 storage needs.  Designed specifically for IBM PS/2 Models 60 and
80, the 155mb and 380mb version provides 100% compatibility with
IBM's ESDI controller card and Reference Diskette and comes
COMPSURFed from the factory.


FEATURES

-High speed data transfer rates and access times.
-Netware, DOS, OS/2 and Xenix compatible.
-Uses system's existing hard disk controller.
-Plug and play installation.





ÿ


MC ENABLER

Procom Technology's ENABLER Series of SCSI Host Adapters for IBM PC,
XT, AT and PS/2 Micro Channel computers enable users to upgrade their
systems to a single interface standard-SCSI.  Providing a full range
of storage and peripheral add-on  option, the Enabers are perfect for
a variety of environments, including DOS and networks.  As storage
needs grow, users can easily and cost effectively expand the storage
capacity fo their PC's without purchasing additional interface cards
or relinguishing valuable expansion slots.

FEATURES
-Dramatically expands the peripheral potential of PC's;  can daisy chain
 up to 7 SCSI devices with each SCSI Enabler.
-High speed data throughput; MC Enabler supports transfer rates up to
 5MB/second.
-Disconnect/reselect fully implemented.
-Compatible with Procom Technology's complete family of SCSI peripherals

ÿ


SCSI Internal Hard Drives

Procom Technology's range of SCSI Enabler Internal 3.5 & 5.25
inch drives are an efficient, cost effective and reliable way to
maximize storage assets for Classic Channel and PS/2 Micro
Channel users.  Providing a path for future upgradability - via
the SCSI interface - without sacrificing Winchester drive
technology, the drives can be daisy chained with up to seven
devics, thus allowing Micro Channel and Classic Channel systems
virtually unlimited storage capability.


Features

-High performance and reliability.
-Drives come COMPSURFed from the factory.
-Powerful, easy-to-use Procom drivers and utility software is
 included with the Enabler host adapters.
-Separate cabling kits are available for each drive alowing for use
 in virtually any Classic Channel or Micro Channel system.
-Sizes range from 45mb to 1000mb ( 1 gigabyte! ).

Accessories Available

PS3 Kit - 3.5" mounting kit for desktop PS/2's.

S5 Kit  - Universal 5.25" kit for XT, AT, Compaq, and PS/2 Model 60,
          65, and 80.
S5H Kit - Universal 5.25" kit for Compaq and compatible systems.


ÿ


MD & MTD External SCSI Hard Disks

Procom Technology's full range of SCSI Enabler External Drives is an
efficient, cost effective and reliable way to maximize storage assets for
Classic Channel and PS/2 Micro Channel users.  Providing a path for future
upgradability--via the SCSI interface--without sacrificing Winchester
drive technology, the drives can be daisy chained with up to 7 devices,
thus allowing Micro Channel systems virtually unlimited storage capability.
Sizes range from 20mb to 650mb

FEATURES
-High performance and reliability.
-Powerful, easy-to-use Procom driver and utility software included.
-External SCSI ID dial and termination switch make the drives easily
 transportable.



ÿ


MRD40

Procom Technology's HIPerformance Removable media SCSI drive offers
Classic Channel and PS/2 Micro Channel computer users a safe and convenient
way to store, transport and back up informaton quickly and easily.  The
advantages of Winchester drive performance have been integrated into the low
profile drive's design while the flexibility of daisy chaining with up to
seven SCSI devices remains, making the drive an ideal choice for users
with high capacity, removable storage needs.

FEATURES
-Fast and reliable removable cartridge technology.
-Virtually unlimited storage capability.
-SCSI ID selection is easy via a simple dial on the rear control panel and
 an external termination switch.



MEOD650

Procom Technology's Erasable Optical Drives are state-of-the-art storage
systems.  Featuring a convenient removable medium, each double-sided
cartridge stores 582 million bytes of data, enabling users to safely
access, archive and transport tremendous data bases.  The drives conform
to ISO/ANSI standards, so data interchangeability among a variety of
cartridge vendors is assured.  All this makes the Erasable Optical Drive
the ideal solution for users with rapidly increasing  storage requirements.

FEATURES
-Up to 582MB of erasable, removable media per cartridge.
-Automatic Bad Block Reallocation helps quarantee the reliablility and
 integrity of the stored data.
-Automatically mounts and unmounts data cartridges as easy as floppy
 diskette drives.
-Ideal for networking and multi-media applications.
-External SCSI address dial and termination switch for easy system
 installation.

ÿ


MCD-ROM 650/E

Procom Technology's HiPerformance CD-ROM drive brings online the
ever-increasing number of CD-based data bases in the market place,
providing users with the ability to access literally millions
of bytes of information in seconds.  And because the drives utilize
the SCSI interface, ISA and Micro Channel computer users can
virtually eliminate storage problems altogether via daisy chaining
withe up to 7 SCSI devices at once.


FEATURES

-External SCSI ID dial and termination switch make installation and setup
 quick and simple.
-Audio and visual output capability when used with most leading 3rd party
 CD-ROM system software.
-Software to play Audio CD's included.
-Low profile design integrates well into almost any home or office
 environment.
-Rated the fastest CD-ROM mechanism on the market by a major computer


  
PMT60/E & PMT150/E


   PRODUCT NOT RELEASED AT THIS TIME.


~~~~~~~~~~~~~~~~~end of capture~~~~~~~~~~~~~~~~~~~












ÿ


MDAT1300/E

Procom Technology's half-height DAT drive is the answer to high
capacity drive users who want a fast and reliable method for
archiving, backing up and transporting important computer data.
Because the DAT drive provides 1.3 Gbytes of storage on a removable
cassette tape about the size of a standard business card, archiving
is safe and simple.  Additionaly the DAT drive can be easily
transported and shared among a variety of SCSI Enabler equipped
computer systems, making it an economic solution for high capacity
archiving and storage needs.

FEATURES
-Fast and efficient operation.
-Conforms to DDS tape standards utilizing R120 tapes.
-External SCSI ID dial and termination switch make installation and
 setup quick and simple.  
-Easy transportable.


ÿ
Bulletin Read : [1 - 68], [L]ist, [N]ew, [Enter] = None : 
