 
AdapterId 0DFAFh
 
AdapterName  "IBM Micro Channel Print Service Adapter."
 
NumBytes 2
 
NamedItem
 
        Prompt "I/O Addresses ........................."
 
        Choice  "0640-0647" pos[0]=XX00000Xb io 0640h-0647h int 7
        Choice  "0648-064F" pos[0]=XX00001Xb io 0648h-064Fh int 7
 
  Help
 
"This option assigns the Print Service Adapter as either
Primary (Addresses 0640h - 0647h) or Secondary (Addresses 0648h - 064Fh).
It is also important to note that the Adapter uses interrupt 7."
 
NamedItem
 
        Prompt "Arbitration level for the Adapter......"
 
        Choice  "Level 1" pos[1]=00000001b arb 1
        Choice  "Level 3" pos[1]=00000011b arb 3
        Choice  "Level 6" pos[1]=00000110b arb 6
        Choice  "Level 7" pos[1]=00000111b arb 7
        Choice  "Level 5" pos[1]=00000101b arb 5
 
 
  Help
 
"This assignment needs to be changed if it is in conflict with
another assignment.  Conflicting assigments are marked with
an asterisk.  Arbitration priorities range from 0 (highest) to
7 (lowest)."
