
AdapterId 05125h

AdapterName "Tecmar QT-60, QT-90, QT-125 Tape Drive"   

NumBytes 2

NamedItem
        Prompt "QT Host Adapter I/O Location"
      choice "I/O 300"    pos[0]=XXXX000Xb  io 0300h-0301h
      choice "I/O 338"    pos[0]=XXXX001Xb  io 0338h-0339h
      choice "I/O 368"    pos[0]=XXXX010Xb  io 0368h-0369h
      choice "I/O 398"    pos[0]=XXXX011Xb  io 0398h-0399h
      choice "I/O 200"    pos[0]=XXXX100Xb  io 0200h-0201h
      choice "I/O 238"    pos[0]=XXXX101Xb  io 0238h-0239h
      choice "I/O 310"    pos[0]=XXXX110Xb  io 0310h-0311h

   Help
 "This port can be assigned to any of seven (7) I/O locations. 
 Use the F5=Previous and the F6=Next keys to change this
 assignment in the 'Change configuration' window.  Conflicting
 assignments are marked with an asterisk and must be changed to
 use the adapter."

NamedItem
        Prompt "QT Host Adapter Interrupt Number"
      choice "Int  3"   pos[0]=XX00XXXXb  int  3
      choice "Int  4"   pos[0]=XX01XXXXb  int  4
      choice "Int  5"   pos[0]=XX10XXXXb  int  5
      choice "Int  6"   pos[0]=XX11XXXXb  int  6
			     
   Help
      "This assignment need only be changed if you do not wish certain
      programs to share interrupts. Use the F5=Previous and the F6=Next keys
      to change arbitration level assignments if you are in the
      'Change configuration' window."

NamedItem
        Prompt "QT Host Adapter DMA Arbitration"
      choice "Level 1"   pos[1]=XXXX0001b  arb  1
      choice "Level 2"   pos[1]=XXXX0010b  arb  2
      choice "Level 3"   pos[1]=XXXX0011b  arb  3
      choice "Level 5"   pos[1]=XXXX0101b  arb  5
      choice "Level 6"   pos[1]=XXXX0110b  arb  6
      choice "Level 7"   pos[1]=XXXX0111b  arb  7
      choice "Level 0"   pos[1]=XXXX0000b  arb  0
      choice "Level 4"   pos[1]=XXXX0100b  arb  4


  Help
      "This assignment need only be changed if it is in conflict
      with another assignment.  Conflicting assignments are marked
      with an asterisk.  Use the F5=Previous and the F6=Next keys
      to change arbitration level assignments if you are in the
      'Change configuration' window."
