
AdapterID 0FDDFh

AdapterName "Enhanced 80386 Memory Expansion Adapter"

Numbytes 4

FixedResources
  POS[0]=000000x0b
  POS[1]=00000000b
  POS[2]=00000000b
  POS[3]=00xxxxxxb Exec


InitProg 31

NamedItem Prompt "Matched Memory Cycles"
          Choice  "Enabled"    pos[0]=XXXXXX1Xb
          Choice  "Disabled"   pos[0]=XXXXXX0Xb

          Help
          "This memory card can disable Matched Memory Cycles for
           use on machines which do not have Matched Memory Cycles
           compatible with the original 16MHz Model-80."

NamedItem Prompt "Enabled Memory"
          Choice  "Run Set Configuration"   pos[3]=xx111111b
          Choice  "0KB (0MB)"         pos[3]=xx000000b
          Choice  "1024KB (1.0MB)"    pos[3]=xx000001b
          Choice  "2048KB (2.0MB)"    pos[3]=xx000010b
          Choice  "3072KB (3.0MB)"    pos[3]=xx000011b
          Choice  "4096KB (4.0MB)"    pos[3]=xx000100b
          Choice  "5120KB (5.0MB)"    pos[3]=xx000101b
          Choice  "6144KB (6.0MB)"    pos[3]=xx000110b
          Choice  "7168KB (7.0MB)"    pos[3]=xx000111b
          Choice  "8192KB (8.0MB)"    pos[3]=xx001000b
          Choice  "9216KB (9.0MB)"    pos[3]=xx001001b
          Choice  "10240KB (10.0MB)"  pos[3]=xx001010b
          Choice  "11264KB (11.0MB)"  pos[3]=xx001011b
          Choice  "12288KB (12.0MB)"  pos[3]=xx001100b
          Choice  "13312KB (13.0MB)"  pos[3]=xx001101b
          Choice  "14336KB (14.0MB)"  pos[3]=xx001110b
          Choice  "15360KB (15.0MB)"  pos[3]=xx001111b
          Choice  "16384KB (16.0MB)"  pos[3]=xx010000b
          Help
          "This item is used to allow the amount of enabled memory
           on the memory card to be displayed when the configuration
           is viewed. Modifying this field does not affect the amount
           of enabled memory on the memory card.

           This entry shows the amount of memory that can be enabled
           on the adapter. Since the total system memory cannot exceed
           16 megs, some of this memory may not be enabled.

           If 'Run Set Configuration' appears in the display,
           Set Configuration must be run again to re-display
           the amount of enabled memory."

