AdapterId 0611Bh

AdapterName "LaserMaster Controller"

NumBytes 4

FixedResources

         pos[0] = xxxx1xx1b
         pos[1] = xxxxxxxxb
         pos[2] = xxxxxxxxb
         pos[3] = xxxx1010b

NamedItem

       Prompt "I/O Address Assignment"

       Choice  "280H"

         pos[1] = 10000000b
         pos[2] = 00000010b
         io 0280h - 028Fh

       Choice  "180H"

         pos[1] = 10000000b
         pos[2] = 00000001b
         io 0180h - 018Fh

   Help

      "Select an I/O address that does not 
      conflict with other adapters in the system."

NamedItem

       Prompt "Interrupt Level Assignment"

       Choice  "Level 3"

         pos[0] = xxxxx00xb
         int 3

       Choice  "Level 4"

         pos[0] = xxxxx01xb
         int 4

       Choice  "Level 7"

         pos[0] = xxxxx10xb
         int 7

       Choice  "Level 9"

         pos[0] = xxxxx11xb
         int 9

   Help

      "Select an Interrupt Level that does not 
      conflict with other adapters in the system."
