AdapterId 06DE7h

AdapterName "Sync-Up 2/208/201"

NumBytes 1

NamedItem 
	Prompt "Synchronous Modem Port" 
      choice "Sync-Up_1"	pos[0]=010xx00xb io 0300h-030fh int 3 
      choice "Sync-Up_2"	pos[0]=011xx00xb io 0300h-030fh int 4 
      choice "Sync-Up_3"	pos[0]=010xx01xb io 0310h-031fh int 3 
      choice "Sync-Up_4"	pos[0]=011xx01xb io 0310h-031fh int 4 
      choice "Sync-Up_5"	pos[0]=010xx10xb io 0340h-034fh int 3 
      choice "Sync-Up_6"	pos[0]=011xx10xb io 0340h-034fh int 4 
      choice "Sync-Up_7"	pos[0]=010xx11xb io 0360h-036fh int 3 
      choice "Sync-Up_8"	pos[0]=011xx11xb io 0360h-036fh int 4 
      choice "DISABLED" 	pos[0]=000xx00xb 
 
Help 
"The Synchronous portion of this modem 
can be assigned to use Sync-Up_1 through Sync-Up_8 or 
DISABLED.  
Use the F5=Previous and the F6=Next keys to change 
the assigment.  Conflicting assignments are 
marked with an asterisk and must be changed." 
