
AdapterId 08202h

AdapterName "AHEAD SYSTEMS INC., VGA ENHANCER-Z, Rev. A"

NumBytes 2

NamedItem
        Prompt "VGA Enhancer-Z  Disable"
      choice "DISABLE" pos[0]=XXXXXXX0b
      choice "ENABLE " pos[0]=XXXXXXX1b

   Help
"This VGA Enhancer-Z card can be either DISABLE or ENABLE.
Use the F5=Previous and the F6=Next keys to change this
assignment in the 'Change configuration' window.  Conflicting
assignments are marked with an asterisk and must be changed to
use the adapter."

NamedItem
        Prompt "Video BIOS ROM Address Select"
      choice "BIOS size= 16K starting @C000h" pos[3]=XXXX0XX1b mem 0C0000h-0C3fffh
      choice "DISABLE BIOS " pos[3]=XXXXXXX0b 
      choice "BIOS size= 8K starting @C000h" pos[3]=XXXX1XX1b mem 0C0000h-0C1fffh

   Help
"The EPROM size can be either 8K (2764) or 16K (27128) or disabled.
Use the F5=Previous and the F6=Next keys to change this
assignment in the 'Change configuration' window.  Conflicting
assignments are marked with an asterisk and must be changed to
use the adapter."
















