AdapterId	060C9H

AdapterName "Boca Research Bidirectional Parallel Adapter"

NumBytes 1

NamedItem

	Prompt "Parallel Connector"

	choice "PARALLEL_1" pos[0]=XX11101Xb    io 03bch-03bfh  int 7
	choice "PARALLEL_2" pos[0]=XX11010Xb    io 0378h-037bh  int 7
	choice "PARALLEL_3" pos[0]=XX10010Xb    io 0278h-027bh  int 7

Help
"This is an IBM compatible bidirectional parallel port.  It may be
configured at any of the three standard port addresses.  You should
configure this card numerically as the next parallel card in the
system.  (ie.  If the system board is PARALLEL_1, and this is the
second parallel board in the system, then choose the PARALLEL_2
option)."

NamedItem

	Prompt "Direction"

	choice "Unidirectional" pos[0]=1XXXXXXXb
	choice "Bidirectional"  pos[0]=0XXXXXXXb

Help
"This board is an IBM compatible bidirectional parallel port.  It may be
placed in either the bidirectional (input/output) or unidirectional (output
only) mode.  The default for the IBM adapter is the unidirectional mode."
