
AdapterId 07fd5h

AdapterName "The NCI 4700 PCI/MC"

NumBytes 1

FixedResources
         pos[0]=XXXXXX0Xb
         io 0220h-022Fh 02D0h-02DFh
         int 2
         mem 0CC000h-0CFFFFh

NamedItem

    Prompt "Adapter Feature selection"
         Choice "REMOTE IPL"
              pos[0]=XXX1XXXXb
         Choice "LOCAL IPL"
              pos[0]=XXX0XXXXb

    Help
        "REMOTE IPl means to Boot the system from the 4702.
         LOCAL IPL means to Boot the system from the local hard disk."

NamedItem

    Prompt "Adapter Feature selection"
         Choice "DISKETTE ENABLE"
              pos[0]=XX0XXXXXb
         Choice "DISKETTE DISABLE"
              pos[0]=XX1XXXXXb

    Help
        "DISKETTE ENABLE means that the diskette drives are available if
         present.
         DISKETTE DISABLE means the diskette drives are disabled and
         not available to be used."

NamedItem

    Prompt "Adapter Feature selection"
         Choice "PRIMARY DOS"
              pos[0]=X1XXXXXXb
         Choice "SECONDARY DOS"
              pos[0]=X0XXXXXXb

    Help
        "PRIMARY DOS means to boot the system as if there were no dual
         DOS system. SECONDARY DOS means to boot the system from the
         secondary DOS system on the remote reset volume."

NamedItem

    Prompt "Adapter Feature selection"
         Choice "IPL override"
              pos[0]=1XXXXXXXb
         Choice "No IPL override"
              pos[0]=0XXXXXXXb


    Help
        "If IPL Override is in effect, the operator will be prompted
         to press the F1 key to override the IPL selection. If No IPL
         Override is specified, the F1 option is not offered."


