AdapterId 06147h

AdapterName "Micro Channel Compatible Key Card"

NumBytes 1

NamedItem

Prompt "Micro Channel Compatible Key Card Addresses"

choice "230h"  pos[0]=XXXX001Xb IO 230h-230h
choice "320h"  pos[0]=XXXX010Xb IO 320h-320h
choice "340h"  pos[0]=XXXX011Xb IO 340h-340h
choice "4230h"  pos[0]=XXXX100Xb IO 4230h-4230h
choice "4320h"  pos[0]=XXXX101Xb IO 4320h-4320h
choice "4340h"  pos[0]=XXXX110Xb IO 4340h-4340h
choice "4888h"  pos[0]=XXXX111Xb IO 4888h-4888h

   Help
"Use the F5=Previous, F6=Next keys to 
change the I/O address of the Micro Channel Compatible Key Card
if you are in the 'Change configuration' window.
Conflicting assignments are marked with an asterisk and
must be changed to use the adapter."


