
AdapterId 07411h

AdapterName "Quadboard PS/Q Multifunction adapter (primary ID)"

NumBytes 6

FixedResources
		pos[3] = 1XXXXX00b

InitProg 30

NamedItem
	Prompt "Parallel Port"
      choice "PARALLEL_1 "  pos[0]=X00XXXXXb  io 03BCh-03Bfh  int 7
      choice "PARALLEL_2 "  pos[0]=X01XXXXXb  io 0378h-037fh  int 7
      choice "PARALLEL_3 "  pos[0]=X10XXXXXb  io 0278h-027fh  int 7
      choice "DISABLED"     pos[0]=X11XXXXXb
   Help
"The parallel port on the Quadboard PS/Q Adapter can be
assigned to use Parallel 1 through Parallel 3.	If you are
in the 'Change configuration' window, you may use the
F5(Previous) and the F6(Next) keys to change parallel port
assignments.  Conflicting assignments are marked with an
asterisk and must be changed to use the adapter."

NamedItem
	Prompt "Parallel Port Mode"
      choice "COMPATIBLE "  pos[0]=1XXXXXXXb
      choice "EXTENDED   "  pos[0]=0XXXXXXXb
   Help
"The Parallel Port can be configured in either COMPATIBLE or
EXTENDED modes.  Selection of the EXTENDED mode allows the
data port to be used as a bidirectional port.  If you are in
the 'Change configuration' window, you may use the
F5(Previous) and the F6(Next) keys to change parallel port
modes.	An automatic configuration will result in an
COMPATIBLE MODE default."


NamedItem
	Prompt "Serial Port "
      choice "SERIAL_1"  pos[0]=XXX0000Xb  io 03f8h-03ffh  int 4
      choice "SERIAL_2"  pos[0]=XXX0001Xb  io 02f8h-02ffh  int 3
      choice "SERIAL_3"  pos[0]=XXX0010Xb  io 3220h-3227h  int 3
      choice "SERIAL_4"  pos[0]=XXX0011Xb  io 3228h-322fh  int 3
      choice "SERIAL_5"  pos[0]=XXX0100Xb  io 4220h-4227h  int 3
      choice "SERIAL_6"  pos[0]=XXX0101Xb  io 4228h-422fh  int 3
      choice "SERIAL_7"  pos[0]=XXX0110Xb  io 5220h-5227h  int 3
      choice "DISABLED"  pos[0]=XXX1111Xb
   Help
"The serial port on the Quadboard PS/Q Adapter can be
assigned to use Serial 1 through Serial 7.  If you are in
the 'Change configuration' window, you may use the
F5(Previous) and the F6(Next) keys to change serial port
assignments.  Conflicting assignments are marked with an
asterisk and must be changed to use the adapter."

