; 
;	$Revision:   1.0  $
;	$Date:   21 Apr 1989 10:58:22  $
; 
;***************************************************************************
;* Copyright (C) 1988 by Phoenix Technologies Ltd.  			   *
;* Copyright (C) 1989 by NCR Corporation    This program		   *
;* contains proprietary and confidential information.  All rights reserved *
;* except as may be permitted by prior written consent.                    *
;*************************************************************************** 
; SYS0100.ADF

; If the configuration file has no NOSHADOW flag then this file will be
; parsed in and displayed.

; Let SETUP know this will require a valid CMOS signature to have effect
PSignature

;******************************************************************
; Extended CMOS 700h - BIOS information.
;        FFh = Shadow BIOS ROM
;        00h = No Shadowing
;******************************************************************
NamedItem
        ECmos 700h
	Prompt "Phoenix ROM BIOS shadowing"
	Choice "Enabled"  pos[0]=11111111b
	Choice "Disabled" pos[0]=00000000b
	Help
"If BIOS ROM shadowing is enabled, the Phoenix ROM BIOS will attempt to
execute from a copy of itself in RAM. Since the RAM is faster than ROM,
programs that use BIOS functions will subsequently execute faster."


